Copyright (c) 1992-2021 The FreeBSD Project.
Copyright (c) 1979, 1980, 1983, 1986, 1988, 1989, 1991, 1992, 1993, 1994
	The Regents of the University of California. All rights reserved.
FreeBSD is a registered trademark of The FreeBSD Foundation.
FreeBSD 12.2-STABLE plus-RELENG_21_05-n202558-698cc2089f8e pfSense amd64
FreeBSD clang version 10.0.1 (git@github.com:llvm/llvm-project.git llvmorg-10.0.1-0-gef32c611aa2)
VT(vga): resolution 640x480
CPU: Intel(R) Atom(TM) CPU C3558 @ 2.20GHz (2200.07-MHz K8-class CPU)
  Origin="GenuineIntel"  Id=0x506f1  Family=0x6  Model=0x5f  Stepping=1
  Features=0xbfebfbff<FPU,VME,DE,PSE,TSC,MSR,PAE,MCE,CX8,APIC,SEP,MTRR,PGE,MCA,CMOV,PAT,PSE36,CLFLUSH,DTS,ACPI,MMX,FXSR,SSE,SSE2,SS,HTT,TM,PBE>
  Features2=0x4ff8ebbf<SSE3,PCLMULQDQ,DTES64,MON,DS_CPL,VMX,EST,TM2,SSSE3,SDBG,CX16,xTPR,PDCM,SSE4.1,SSE4.2,x2APIC,MOVBE,POPCNT,TSCDLT,AESNI,XSAVE,OSXSAVE,RDRAND>
  AMD Features=0x2c100800<SYSCALL,NX,Page1GB,RDTSCP,LM>
  AMD Features2=0x101<LAHF,Prefetch>
  Structured Extended Features=0x2294e283<FSGSBASE,TSCADJ,SMEP,ERMS,NFPUSG,MPX,PQE,RDSEED,SMAP,CLFLUSHOPT,PROCTRACE,SHA>
  Structured Extended Features3=0xac000400<MD_CLEAR,IBPB,STIBP,ARCH_CAP,SSBD>
  XSAVE Features=0xf<XSAVEOPT,XSAVEC,XINUSE,XSAVES>
  IA32_ARCH_CAPS=0x69<RDCL_NO,SKIP_L1DFL_VME>
  VT-x: PAT,HLT,MTF,PAUSE,EPT,UG,VPID,VID,PostIntr
  TSC: P-state invariant, performance statistics
real memory  = 8589934592 (8192 MB)
avail memory = 8157822976 (7779 MB)
Event timer "LAPIC" quality 600
ACPI APIC Table: <INSYDE H2O BIOS>
WARNING: L1 data cache covers fewer APIC IDs than a core (0 < 1)
FreeBSD/SMP: Multiprocessor System Detected: 4 CPUs
FreeBSD/SMP: 1 package(s) x 4 core(s)
arc4random: no preloaded entropy cache
ioapic0 <Version 2.0> irqs 0-119 on motherboard
Launching APs: 1 2 3
Timecounter "TSC-low" frequency 1100035087 Hz quality 1000
wlan: mac acl policy registered
random: entropy device external interface
ipw_bss: You need to read the LICENSE file in /usr/share/doc/legal/intel_ipw.LICENSE.
ipw_bss: If you agree with the license, set legal.intel_ipw.license_ack=1 in /boot/loader.conf.
module_register_init: MOD_LOAD (ipw_bss_fw, 0xffffffff8073c7e0, 0) error 1
ipw_ibss: You need to read the LICENSE file in /usr/share/doc/legal/intel_ipw.LICENSE.
ipw_ibss: If you agree with the license, set legal.intel_ipw.license_ack=1 in /boot/loader.conf.
module_register_init: MOD_LOAD (ipw_ibss_fw, 0xffffffff8073c890, 0) error 1
ipw_monitor: You need to read the LICENSE file in /usr/share/doc/legal/intel_ipw.LICENSE.
ipw_monitor: If you agree with the license, set legal.intel_ipw.license_ack=1 in /boot/loader.conf.
module_register_init: MOD_LOAD (ipw_monitor_fw, 0xffffffff8073c940, 0) error 1
iwi_bss: You need to read the LICENSE file in /usr/share/doc/legal/intel_iwi.LICENSE.
iwi_bss: If you agree with the license, set legal.intel_iwi.license_ack=1 in /boot/loader.conf.
module_register_init: MOD_LOAD (iwi_bss_fw, 0xffffffff807641d0, 0) error 1
iwi_ibss: You need to read the LICENSE file in /usr/share/doc/legal/intel_iwi.LICENSE.
iwi_ibss: If you agree with the license, set legal.intel_iwi.license_ack=1 in /boot/loader.conf.
module_register_init: MOD_LOAD (iwi_ibss_fw, 0xffffffff80764280, 0) error 1
iwi_monitor: You need to read the LICENSE file in /usr/share/doc/legal/intel_iwi.LICENSE.
iwi_monitor: If you agree with the license, set legal.intel_iwi.license_ack=1 in /boot/loader.conf.
module_register_init: MOD_LOAD (iwi_monitor_fw, 0xffffffff80764330, 0) error 1
WARNING: Device "g_ctl" is Giant locked and may be deleted before FreeBSD 14.0.
000.000018 [4344] netmap_init               netmap: loaded module
WARNING: Device "pci" is Giant locked and may be deleted before FreeBSD 14.0.
module_register_init: MOD_LOAD (vesa, 0xffffffff814060c0, 0) error 19
WARNING: Device "kbd" is Giant locked and may be deleted before FreeBSD 14.0.
kbd0 at kbdmux0
random: registering fast source Intel Secure Key RNG
random: fast provider: "Intel Secure Key RNG"
WARNING: Device "spkr" is Giant locked and may be deleted before FreeBSD 14.0.
[ath_hal] loaded
mlx5en: Mellanox Ethernet driver 3.6.0 (December 2020)
nexus0
efirtc0: <EFI Realtime Clock> on motherboard
efirtc0: registered as a time-of-day clock, resolution 1.000000s
vtvga0: <VT VGA driver> on motherboard
cryptosoft0: <software crypto> on motherboard
acpi0: <INSYDE H2O BIOS> on motherboard
acpi0: Power Button (fixed)
unknown: I/O range not supported
cpu0: <ACPI CPU> on acpi0
hpet0: <High Precision Event Timer> iomem 0xfed00000-0xfed003ff on acpi0
Timecounter "HPET" frequency 24000000 Hz quality 950
Event timer "HPET" frequency 24000000 Hz quality 550
Event timer "HPET1" frequency 24000000 Hz quality 440
Event timer "HPET2" frequency 24000000 Hz quality 440
Event timer "HPET3" frequency 24000000 Hz quality 440
Event timer "HPET4" frequency 24000000 Hz quality 440
atrtc0: <AT realtime clock> port 0x70-0x77 irq 8 on acpi0
atrtc0: Warning: Couldn't map I/O.
atrtc0: registered as a time-of-day clock, resolution 1.000000s
Event timer "RTC" frequency 32768 Hz quality 0
attimer0: <AT timer> port 0x40-0x43,0x50-0x53 irq 0 on acpi0
Timecounter "i8254" frequency 1193182 Hz quality 0
Event timer "i8254" frequency 1193182 Hz quality 100
Timecounter "ACPI-fast" frequency 3579545 Hz quality 900
acpi_timer0: <24-bit timer at 3.579545MHz> port 0x1808-0x180b on acpi0
pcib0: <ACPI Host-PCI bridge> port 0xcf8-0xcff on acpi0
pci0: <ACPI PCI bus> on pcib0
pcib1: <ACPI PCI-PCI bridge> at device 6.0 on pci0
pci1: <ACPI PCI bus> on pcib1
pci1: <processor> at device 0.0 (no driver attached)
pcib2: <ACPI PCI-PCI bridge> mem 0x81500000-0x8151ffff at device 10.0 on pci0
pci2: <ACPI PCI bus> on pcib2
pcib3: <ACPI PCI-PCI bridge> mem 0x81520000-0x8153ffff at device 11.0 on pci0
pci3: <ACPI PCI bus> on pcib3
pcib4: <ACPI PCI-PCI bridge> mem 0x81540000-0x8155ffff at device 12.0 on pci0
pci4: <ACPI PCI bus> on pcib4
igc0: <Intel(R) PRO/1000 PCI-Express Network Driver> mem 0x81300000-0x813fffff,0x81400000-0x81403fff at device 0.0 on pci4
igc0: Using 1024 TX descriptors and 1024 RX descriptors
igc0: Using 4 RX queues 4 TX queues
igc0: Using MSI-X interrupts with 5 vectors
igc0: Ethernet address: 90:ec:77:1b:63:55
igc0: netmap queues/slots: TX 4/1024, RX 4/1024
pcib5: <ACPI PCI-PCI bridge> mem 0x81560000-0x8157ffff at device 14.0 on pci0
pci5: <ACPI PCI bus> on pcib5
igc1: <Intel(R) PRO/1000 PCI-Express Network Driver> mem 0x81100000-0x811fffff,0x81200000-0x81203fff at device 0.0 on pci5
igc1: Using 1024 TX descriptors and 1024 RX descriptors
igc1: Using 4 RX queues 4 TX queues
igc1: Using MSI-X interrupts with 5 vectors
igc1: Ethernet address: 90:ec:77:1b:63:56
igc1: netmap queues/slots: TX 4/1024, RX 4/1024
pcib6: <ACPI PCI-PCI bridge> mem 0x81580000-0x8159ffff at device 15.0 on pci0
pci6: <ACPI PCI bus> on pcib6
igc2: <Intel(R) PRO/1000 PCI-Express Network Driver> mem 0x80f00000-0x80ffffff,0x81000000-0x81003fff at device 0.0 on pci6
igc2: Using 1024 TX descriptors and 1024 RX descriptors
igc2: Using 4 RX queues 4 TX queues
igc2: Using MSI-X interrupts with 5 vectors
igc2: Ethernet address: 90:ec:77:1b:63:57
igc2: netmap queues/slots: TX 4/1024, RX 4/1024
pcib7: <ACPI PCI-PCI bridge> mem 0x815a0000-0x815bffff at device 16.0 on pci0
pci7: <ACPI PCI bus> on pcib7
igc3: <Intel(R) PRO/1000 PCI-Express Network Driver> mem 0x80d00000-0x80dfffff,0x80e00000-0x80e03fff at device 0.0 on pci7
igc3: Using 1024 TX descriptors and 1024 RX descriptors
igc3: Using 4 RX queues 4 TX queues
igc3: Using MSI-X interrupts with 5 vectors
igc3: Ethernet address: 90:ec:77:1b:63:58
igc3: netmap queues/slots: TX 4/1024, RX 4/1024
pcib8: <ACPI PCI-PCI bridge> mem 0x815c0000-0x815dffff at device 17.0 on pci0
pci8: <ACPI PCI bus> on pcib8
xhci0: <Intel Denverton USB 3.0 controller> mem 0x815e0000-0x815effff at device 21.0 on pci0
xhci0: 32 bytes context size, 64-bit DMA
usbus0 on xhci0
usbus0: 5.0Gbps Super Speed USB v3.0
pcib9: <ACPI PCI-PCI bridge> at device 22.0 on pci0
pci9: <ACPI PCI bus> on pcib9
ix0: <Intel(R) PRO/10GbE PCI-Express Network Driver> mem 0x80400000-0x805fffff,0x80604000-0x80607fff at device 0.0 on pci9
ix0: Using 2048 TX descriptors and 2048 RX descriptors
ix0: Using 4 RX queues 4 TX queues
ix0: Using MSI-X interrupts with 5 vectors
ix0: allocated for 4 queues
ix0: allocated for 4 rx queues
ix0: Ethernet address: 90:ec:77:1b:63:53
ix0: netmap queues/slots: TX 4/2048, RX 4/2048
ix1: <Intel(R) PRO/10GbE PCI-Express Network Driver> mem 0x80200000-0x803fffff,0x80600000-0x80603fff at device 0.1 on pci9
ix1: Using 2048 TX descriptors and 2048 RX descriptors
ix1: Using 4 RX queues 4 TX queues
ix1: Using MSI-X interrupts with 5 vectors
ix1: allocated for 4 queues
ix1: allocated for 4 rx queues
ix1: Ethernet address: 90:ec:77:1b:63:54
ix1: netmap queues/slots: TX 4/2048, RX 4/2048
pcib10: <ACPI PCI-PCI bridge> at device 23.0 on pci0
pci10: <ACPI PCI bus> on pcib10
ix2: <Intel(R) PRO/10GbE PCI-Express Network Driver> mem 0x80a00000-0x80bfffff,0x80c04000-0x80c07fff at device 0.0 on pci10
ix2: Using 2048 TX descriptors and 2048 RX descriptors
ix2: Using 4 RX queues 4 TX queues
ix2: Using MSI-X interrupts with 5 vectors
ix2: allocated for 4 queues
ix2: allocated for 4 rx queues
ix2: Ethernet address: 90:ec:77:1b:63:52
ix2: netmap queues/slots: TX 4/2048, RX 4/2048
ix3: <Intel(R) PRO/10GbE PCI-Express Network Driver> mem 0x80800000-0x809fffff,0x80c00000-0x80c03fff at device 0.1 on pci10
ix3: Using 2048 TX descriptors and 2048 RX descriptors
ix3: Using 4 RX queues 4 TX queues
ix3: Using MSI-X interrupts with 5 vectors
ix3: allocated for 4 queues
ix3: allocated for 4 rx queues
ix3: Ethernet address: 90:ec:77:1b:63:51
ix3: netmap queues/slots: TX 4/2048, RX 4/2048
pci0: <simple comms> at device 24.0 (no driver attached)
sdhci_pci0: <Intel Denverton eMMC 5.0 Controller> mem 0x815f6000-0x815f6fff,0x815f7000-0x815f7fff at device 28.0 on pci0
sdhci_pci0: 1 slot(s) allocated
mmc0: <MMC/SD bus> on sdhci_pci0
isab0: <PCI-ISA bridge> at device 31.0 on pci0
isa0: <ISA bus> on isab0
pci0: <memory> at device 31.2 (no driver attached)
pci0: <serial bus> at device 31.5 (no driver attached)
pci0: <unknown> at device 31.7 (no driver attached)
acpi_button0: <Power Button> on acpi0
acpi_tz0: <Thermal Zone> on acpi0
uart0: <Non-standard ns8250 class UART with FIFOs> port 0x3f8-0x3ff irq 16 flags 0x10 on acpi0
uart0: console (115200,n,8,1)
est0: <Enhanced SpeedStep Frequency Control> on cpu0
Timecounters tick every 1.000 msec
arc4random: no preloaded entropy cache
ugen0.1: <0x8086 XHCI root HUB> at usbus0
uhub0: <0x8086 XHCI root HUB, class 9/0, rev 3.00/1.00, addr 1> on usbus0
mmcsd0: 16GB <MMCHC TB2916 9.0 SN 28E9724C MFG 09/2020 by 112 0x0000> at mmc0 50.0MHz/8bit/65535-block
mmcsd0boot0: 4MB partition 1 at mmcsd0
mmcsd0boot1: 4MB partition 2 at mmcsd0
mmcsd0rpmb: 4MB partition 3 at mmcsd0
Trying to mount root from ufs:/dev/ufsid/60b9302175a9865b [rw,noatime]...
random: unblocking device.
arc4random: no preloaded entropy cache
arc4random: no preloaded entropy cache
Netgate 6100 GPIO Driver 0.3 loaded
cordbuc0: <Netgate 6100 IO controller> at port 0x800 on isa0
gpio0: <SG-6100 uC GPIO controller> on cordbuc0
gpiobus0: <GPIO bus> on gpio0
gpioled0: <GPIO led> at pin 0 on gpiobus0
gpioled1: <GPIO led> at pin 1 on gpiobus0
gpioled10: <GPIO led> at pin 10 on gpiobus0
gpioled11: <GPIO led> at pin 11 on gpiobus0
gpioled2: <GPIO led> at pin 2 on gpiobus0
gpioled3: <GPIO led> at pin 3 on gpiobus0
gpioled4: <GPIO led> at pin 4 on gpiobus0
gpioled5: <GPIO led> at pin 5 on gpiobus0
gpioled6: <GPIO led> at pin 6 on gpiobus0
gpioled7: <GPIO led> at pin 7 on gpiobus0
gpioled8: <GPIO led> at pin 8 on gpiobus0
gpioled9: <GPIO led> at pin 9 on gpiobus0
gpioc0: <GPIO controller> on gpio0
uhub0: 8 ports with 8 removable, self powered
CPU: Intel(R) Atom(TM) CPU C3558 @ 2.20GHz (2200.07-MHz K8-class CPU)
  Origin="GenuineIntel"  Id=0x506f1  Family=0x6  Model=0x5f  Stepping=1
  Features=0xbfebfbff<FPU,VME,DE,PSE,TSC,MSR,PAE,MCE,CX8,APIC,SEP,MTRR,PGE,MCA,CMOV,PAT,PSE36,CLFLUSH,DTS,ACPI,MMX,FXSR,SSE,SSE2,SS,HTT,TM,PBE>
  Features2=0x4ff8ebbf<SSE3,PCLMULQDQ,DTES64,MON,DS_CPL,VMX,EST,TM2,SSSE3,SDBG,CX16,xTPR,PDCM,SSE4.1,SSE4.2,x2APIC,MOVBE,POPCNT,TSCDLT,AESNI,XSAVE,OSXSAVE,RDRAND>
  AMD Features=0x2c100800<SYSCALL,NX,Page1GB,RDTSCP,LM>
  AMD Features2=0x101<LAHF,Prefetch>
  Structured Extended Features=0x2294e283<FSGSBASE,TSCADJ,SMEP,ERMS,NFPUSG,MPX,PQE,RDSEED,SMAP,CLFLUSHOPT,PROCTRACE,SHA>
  Structured Extended Features3=0xac000400<MD_CLEAR,IBPB,STIBP,ARCH_CAP,SSBD>
  XSAVE Features=0xf<XSAVEOPT,XSAVEC,XINUSE,XSAVES>
  IA32_ARCH_CAPS=0x69<RDCL_NO,SKIP_L1DFL_VME>
  VT-x: PAT,HLT,MTF,PAUSE,EPT,UG,VPID,VID,PostIntr
  TSC: P-state invariant, performance statistics
