[    0.000000] microcode: microcode updated early to revision 0x34, date = 2020-10-23
[    0.000000] Linux version 5.4.0-90-generic (buildd@lgw01-amd64-054) (gcc version 9.3.0 (Ubuntu 9.3.0-17ubuntu1~20.04)) #101-Ubuntu SMP Fri Oct 15 20:00:55 UTC 2021 (Ubuntu 5.4.0-90.101-generic 5.4.148)
[    0.000000] Command line: BOOT_IMAGE=/boot/vmlinuz-5.4.0-90-generic root=UUID=fb875ad8-746f-48b7-a1c4-c19fc4a7d3ff ro console=ttyS0,115200n8 isolcpu=1-3
[    0.000000] KERNEL supported cpus:
[    0.000000]   Intel GenuineIntel
[    0.000000]   AMD AuthenticAMD
[    0.000000]   Hygon HygonGenuine
[    0.000000]   Centaur CentaurHauls
[    0.000000]   zhaoxin   Shanghai  
[    0.000000] x86/fpu: Supporting XSAVE feature 0x001: 'x87 floating point registers'
[    0.000000] x86/fpu: Supporting XSAVE feature 0x002: 'SSE registers'
[    0.000000] x86/fpu: Supporting XSAVE feature 0x008: 'MPX bounds registers'
[    0.000000] x86/fpu: Supporting XSAVE feature 0x010: 'MPX CSR'
[    0.000000] x86/fpu: xstate_offset[3]:  576, xstate_sizes[3]:   64
[    0.000000] x86/fpu: xstate_offset[4]:  640, xstate_sizes[4]:   64
[    0.000000] x86/fpu: Enabled xstate features 0x1b, context size is 704 bytes, using 'compacted' format.
[    0.000000] BIOS-provided physical RAM map:
[    0.000000] BIOS-e820: [mem 0x0000000000000000-0x000000000005efff] usable
[    0.000000] BIOS-e820: [mem 0x000000000005f000-0x000000000005ffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000000060000-0x000000000009ffff] usable
[    0.000000] BIOS-e820: [mem 0x00000000000a0000-0x00000000000fffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000000100000-0x000000007c2befff] usable
[    0.000000] BIOS-e820: [mem 0x000000007c2bf000-0x000000007ebbefff] reserved
[    0.000000] BIOS-e820: [mem 0x000000007ebbf000-0x000000007efbefff] ACPI NVS
[    0.000000] BIOS-e820: [mem 0x000000007efbf000-0x000000007effefff] ACPI data
[    0.000000] BIOS-e820: [mem 0x000000007efff000-0x000000007effffff] usable
[    0.000000] BIOS-e820: [mem 0x000000007f000000-0x000000007fffffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000e0000000-0x00000000efffffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fd000000-0x00000000fe7fffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fec00000-0x00000000fec00fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fec80000-0x00000000fed00fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fed10000-0x00000000fed17fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fed84000-0x00000000fed84fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000ff800000-0x00000000ffffffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000100000000-0x000000027fffffff] usable
[    0.000000] NX (Execute Disable) protection: active
[    0.000000] e820: update [mem 0x72008018-0x72039657] usable ==> usable
[    0.000000] e820: update [mem 0x72008018-0x72039657] usable ==> usable
[    0.000000] e820: update [mem 0x71fd6018-0x72007657] usable ==> usable
[    0.000000] e820: update [mem 0x71fd6018-0x72007657] usable ==> usable
[    0.000000] e820: update [mem 0x71fa4018-0x71fd5657] usable ==> usable
[    0.000000] e820: update [mem 0x71fa4018-0x71fd5657] usable ==> usable
[    0.000000] e820: update [mem 0x71f72018-0x71fa3657] usable ==> usable
[    0.000000] e820: update [mem 0x71f72018-0x71fa3657] usable ==> usable
[    0.000000] extended physical RAM map:
[    0.000000] reserve setup_data: [mem 0x0000000000000000-0x000000000005efff] usable
[    0.000000] reserve setup_data: [mem 0x000000000005f000-0x000000000005ffff] reserved
[    0.000000] reserve setup_data: [mem 0x0000000000060000-0x000000000009ffff] usable
[    0.000000] reserve setup_data: [mem 0x00000000000a0000-0x00000000000fffff] reserved
[    0.000000] reserve setup_data: [mem 0x0000000000100000-0x0000000071f72017] usable
[    0.000000] reserve setup_data: [mem 0x0000000071f72018-0x0000000071fa3657] usable
[    0.000000] reserve setup_data: [mem 0x0000000071fa3658-0x0000000071fa4017] usable
[    0.000000] reserve setup_data: [mem 0x0000000071fa4018-0x0000000071fd5657] usable
[    0.000000] reserve setup_data: [mem 0x0000000071fd5658-0x0000000071fd6017] usable
[    0.000000] reserve setup_data: [mem 0x0000000071fd6018-0x0000000072007657] usable
[    0.000000] reserve setup_data: [mem 0x0000000072007658-0x0000000072008017] usable
[    0.000000] reserve setup_data: [mem 0x0000000072008018-0x0000000072039657] usable
[    0.000000] reserve setup_data: [mem 0x0000000072039658-0x000000007c2befff] usable
[    0.000000] reserve setup_data: [mem 0x000000007c2bf000-0x000000007ebbefff] reserved
[    0.000000] reserve setup_data: [mem 0x000000007ebbf000-0x000000007efbefff] ACPI NVS
[    0.000000] reserve setup_data: [mem 0x000000007efbf000-0x000000007effefff] ACPI data
[    0.000000] reserve setup_data: [mem 0x000000007efff000-0x000000007effffff] usable
[    0.000000] reserve setup_data: [mem 0x000000007f000000-0x000000007fffffff] reserved
[    0.000000] reserve setup_data: [mem 0x00000000e0000000-0x00000000efffffff] reserved
[    0.000000] reserve setup_data: [mem 0x00000000fd000000-0x00000000fe7fffff] reserved
[    0.000000] reserve setup_data: [mem 0x00000000fec00000-0x00000000fec00fff] reserved
[    0.000000] reserve setup_data: [mem 0x00000000fec80000-0x00000000fed00fff] reserved
[    0.000000] reserve setup_data: [mem 0x00000000fed10000-0x00000000fed17fff] reserved
[    0.000000] reserve setup_data: [mem 0x00000000fed84000-0x00000000fed84fff] reserved
[    0.000000] reserve setup_data: [mem 0x00000000ff800000-0x00000000ffffffff] reserved
[    0.000000] reserve setup_data: [mem 0x0000000100000000-0x000000027fffffff] usable
[    0.000000] efi: EFI v2.50 by Insyde Mar  5 2021 13:53:37
[    0.000000] efi:  ACPI 2.0=0x7effe014  SMBIOS=0x7c583000  SMBIOS 3.0=0x7c581000 
[    0.000000] secureboot: Secure boot disabled
[    0.000000] SMBIOS 3.0.0 present.
[    0.000000] DMI: Netgate 6100/80500-0214-G01, BIOS CORDOBA-02.01.00.05t 2021-07-25
[    0.000000] tsc: Detected 2200.000 MHz processor
[    0.000024] e820: update [mem 0x00000000-0x00000fff] usable ==> reserved
[    0.000026] e820: remove [mem 0x000a0000-0x000fffff] usable
[    0.000037] last_pfn = 0x280000 max_arch_pfn = 0x400000000
[    0.000042] MTRR default type: uncachable
[    0.000044] MTRR fixed ranges enabled:
[    0.000045]   00000-9FFFF write-back
[    0.000046]   A0000-BFFFF uncachable
[    0.000048]   C0000-E7FFF write-protect
[    0.000049]   E8000-EFFFF write-combining
[    0.000050]   F0000-FFFFF write-protect
[    0.000051] MTRR variable ranges enabled:
[    0.000053]   0 base 00FF800000 mask 7FFF800000 write-protect
[    0.000055]   1 base 0000000000 mask 7F80000000 write-back
[    0.000056]   2 base 007F000000 mask 7FFF000000 uncachable
[    0.000058]   3 base 0100000000 mask 7F00000000 write-back
[    0.000059]   4 base 0200000000 mask 7F80000000 write-back
[    0.000060]   5 disabled
[    0.000061]   6 disabled
[    0.000062]   7 disabled
[    0.000062]   8 disabled
[    0.000063]   9 disabled
[    0.000169] x86/PAT: Configuration [0-7]: WB  WC  UC- UC  WB  WP  UC- WT  
[    0.000336] x2apic: enabled by BIOS, switching to x2apic ops
[    0.000338] last_pfn = 0x7f000 max_arch_pfn = 0x400000000
[    0.005175] check: Scanning 1 areas for low memory corruption
[    0.005184] Using GB pages for direct mapping
[    0.005770] secureboot: Secure boot disabled
[    0.005773] RAMDISK: [mem 0x3ce3a000-0x3fffdfff]
[    0.005782] ACPI: Early table checksum verification disabled
[    0.005789] ACPI: RSDP 0x000000007EFFE014 000024 (v02 INSYDE)
[    0.005793] ACPI: XSDT 0x000000007EFFE120 00007C (v01 INSYDE H2O BIOS 00000001      01000013)
[    0.005802] ACPI: FACP 0x000000007EFF8000 00010C (v05 INSYDE H2O BIOS 00000001 ACPI 00040000)
[    0.005810] ACPI: DSDT 0x000000007EFF0000 004871 (v02 INSYDE H2O BIOS 00000000 ACPI 00040000)
[    0.005815] ACPI: FACS 0x000000007EF86000 000040
[    0.005819] ACPI: UEFI 0x000000007EFFD000 000236 (v01 INSYDE H2O BIOS 00000001 ACPI 00040000)
[    0.005824] ACPI: UEFI 0x000000007EFFB000 000042 (v01                 00000000      00000000)
[    0.005829] ACPI: BDAT 0x000000007EFFA000 000030 (v01 INSYDE H2O BIOS 00000000 ACPI 00040000)
[    0.005834] ACPI: BOOT 0x000000007EFF9000 000028 (v01 INSYDE H2O BIOS 00000001 ACPI 00040000)
[    0.005839] ACPI: HPET 0x000000007EFF7000 000038 (v01 INSYDE H2O BIOS 00000001 ACPI 00040000)
[    0.005843] ACPI: APIC 0x000000007EFF6000 0000D2 (v03 INSYDE H2O BIOS 00000001 ACPI 00040000)
[    0.005848] ACPI: MCFG 0x000000007EFF5000 00003C (v01 INSYDE H2O BIOS 00000001 ACPI 00040000)
[    0.005853] ACPI: SSDT 0x000000007EFEE000 001901 (v02 PmRef  CpuPm    00003000 INTL 20130117)
[    0.005858] ACPI: DMAR 0x000000007EFED000 000070 (v01 INTEL  BDW      00000001 INTL 00000001)
[    0.005862] ACPI: DBG2 0x000000007EFEC000 000061 (v00 INTEL           00000000 MSFT 01000013)
[    0.005867] ACPI: Reserving FACP table memory at [mem 0x7eff8000-0x7eff810b]
[    0.005869] ACPI: Reserving DSDT table memory at [mem 0x7eff0000-0x7eff4870]
[    0.005871] ACPI: Reserving FACS table memory at [mem 0x7ef86000-0x7ef8603f]
[    0.005873] ACPI: Reserving UEFI table memory at [mem 0x7effd000-0x7effd235]
[    0.005875] ACPI: Reserving UEFI table memory at [mem 0x7effb000-0x7effb041]
[    0.005877] ACPI: Reserving BDAT table memory at [mem 0x7effa000-0x7effa02f]
[    0.005878] ACPI: Reserving BOOT table memory at [mem 0x7eff9000-0x7eff9027]
[    0.005880] ACPI: Reserving HPET table memory at [mem 0x7eff7000-0x7eff7037]
[    0.005882] ACPI: Reserving APIC table memory at [mem 0x7eff6000-0x7eff60d1]
[    0.005884] ACPI: Reserving MCFG table memory at [mem 0x7eff5000-0x7eff503b]
[    0.005886] ACPI: Reserving SSDT table memory at [mem 0x7efee000-0x7efef900]
[    0.005888] ACPI: Reserving DMAR table memory at [mem 0x7efed000-0x7efed06f]
[    0.005890] ACPI: Reserving DBG2 table memory at [mem 0x7efec000-0x7efec060]
[    0.005902] ACPI: Local APIC address 0xfee00000
[    0.005905] Setting APIC routing to cluster x2apic.
[    0.006045] No NUMA configuration found
[    0.006047] Faking a node at [mem 0x0000000000000000-0x000000027fffffff]
[    0.006062] NODE_DATA(0) allocated [mem 0x27ffd5000-0x27fffffff]
[    0.006521] Zone ranges:
[    0.006523]   DMA      [mem 0x0000000000001000-0x0000000000ffffff]
[    0.006525]   DMA32    [mem 0x0000000001000000-0x00000000ffffffff]
[    0.006527]   Normal   [mem 0x0000000100000000-0x000000027fffffff]
[    0.006529]   Device   empty
[    0.006531] Movable zone start for each node
[    0.006535] Early memory node ranges
[    0.006537]   node   0: [mem 0x0000000000001000-0x000000000005efff]
[    0.006539]   node   0: [mem 0x0000000000060000-0x000000000009ffff]
[    0.006540]   node   0: [mem 0x0000000000100000-0x000000007c2befff]
[    0.006542]   node   0: [mem 0x000000007efff000-0x000000007effffff]
[    0.006544]   node   0: [mem 0x0000000100000000-0x000000027fffffff]
[    0.006750] Zeroed struct page in unavailable ranges: 15778 pages
[    0.006752] Initmem setup node 0 [mem 0x0000000000001000-0x000000027fffffff]
[    0.006755] On node 0 totalpages: 2081374
[    0.006757]   DMA zone: 64 pages used for memmap
[    0.006758]   DMA zone: 22 pages reserved
[    0.006760]   DMA zone: 3998 pages, LIFO batch:0
[    0.006852]   DMA32 zone: 7883 pages used for memmap
[    0.006854]   DMA32 zone: 504512 pages, LIFO batch:63
[    0.022215]   Normal zone: 24576 pages used for memmap
[    0.022217]   Normal zone: 1572864 pages, LIFO batch:63
[    0.056704] ACPI: PM-Timer IO Port: 0x1808
[    0.056709] ACPI: Local APIC address 0xfee00000
[    0.056723] ACPI: LAPIC_NMI (acpi_id[0xff] high edge lint[0x1])
[    0.056743] IOAPIC[0]: apic_id 2, version 32, address 0xfec00000, GSI 0-119
[    0.056747] ACPI: INT_SRC_OVR (bus 0 bus_irq 0 global_irq 2 dfl dfl)
[    0.056750] ACPI: INT_SRC_OVR (bus 0 bus_irq 9 global_irq 9 high level)
[    0.056753] ACPI: IRQ0 used by override.
[    0.056755] ACPI: IRQ9 used by override.
[    0.056757] Using ACPI (MADT) for SMP configuration information
[    0.056760] ACPI: HPET id: 0x8086a001 base: 0xfed00000
[    0.056769] TSC deadline timer available
[    0.056772] smpboot: Allowing 16 CPUs, 12 hotplug CPUs
[    0.056807] PM: Registered nosave memory: [mem 0x00000000-0x00000fff]
[    0.056811] PM: Registered nosave memory: [mem 0x0005f000-0x0005ffff]
[    0.056814] PM: Registered nosave memory: [mem 0x000a0000-0x000fffff]
[    0.056817] PM: Registered nosave memory: [mem 0x71f72000-0x71f72fff]
[    0.056820] PM: Registered nosave memory: [mem 0x71fa3000-0x71fa3fff]
[    0.056822] PM: Registered nosave memory: [mem 0x71fa4000-0x71fa4fff]
[    0.056825] PM: Registered nosave memory: [mem 0x71fd5000-0x71fd5fff]
[    0.056826] PM: Registered nosave memory: [mem 0x71fd6000-0x71fd6fff]
[    0.056830] PM: Registered nosave memory: [mem 0x72007000-0x72007fff]
[    0.056831] PM: Registered nosave memory: [mem 0x72008000-0x72008fff]
[    0.056834] PM: Registered nosave memory: [mem 0x72039000-0x72039fff]
[    0.056837] PM: Registered nosave memory: [mem 0x7c2bf000-0x7ebbefff]
[    0.056839] PM: Registered nosave memory: [mem 0x7ebbf000-0x7efbefff]
[    0.056840] PM: Registered nosave memory: [mem 0x7efbf000-0x7effefff]
[    0.056843] PM: Registered nosave memory: [mem 0x7f000000-0x7fffffff]
[    0.056845] PM: Registered nosave memory: [mem 0x80000000-0xdfffffff]
[    0.056846] PM: Registered nosave memory: [mem 0xe0000000-0xefffffff]
[    0.056848] PM: Registered nosave memory: [mem 0xf0000000-0xfcffffff]
[    0.056849] PM: Registered nosave memory: [mem 0xfd000000-0xfe7fffff]
[    0.056850] PM: Registered nosave memory: [mem 0xfe800000-0xfebfffff]
[    0.056852] PM: Registered nosave memory: [mem 0xfec00000-0xfec00fff]
[    0.056853] PM: Registered nosave memory: [mem 0xfec01000-0xfec7ffff]
[    0.056855] PM: Registered nosave memory: [mem 0xfec80000-0xfed00fff]
[    0.056856] PM: Registered nosave memory: [mem 0xfed01000-0xfed0ffff]
[    0.056857] PM: Registered nosave memory: [mem 0xfed10000-0xfed17fff]
[    0.056859] PM: Registered nosave memory: [mem 0xfed18000-0xfed83fff]
[    0.056860] PM: Registered nosave memory: [mem 0xfed84000-0xfed84fff]
[    0.056861] PM: Registered nosave memory: [mem 0xfed85000-0xff7fffff]
[    0.056863] PM: Registered nosave memory: [mem 0xff800000-0xffffffff]
[    0.056866] [mem 0x80000000-0xdfffffff] available for PCI devices
[    0.056869] Booting paravirtualized kernel on bare hardware
[    0.056874] clocksource: refined-jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645519600211568 ns
[    0.056887] setup_percpu: NR_CPUS:8192 nr_cpumask_bits:16 nr_cpu_ids:16 nr_node_ids:1
[    0.058627] percpu: Embedded 55 pages/cpu s188416 r8192 d28672 u262144
[    0.058643] pcpu-alloc: s188416 r8192 d28672 u262144 alloc=1*2097152
[    0.058645] pcpu-alloc: [0] 00 01 02 03 04 05 06 07 [0] 08 09 10 11 12 13 14 15 
[    0.058710] Built 1 zonelists, mobility grouping on.  Total pages: 2048829
[    0.058714] Policy zone: Normal
[    0.058717] Kernel command line: BOOT_IMAGE=/boot/vmlinuz-5.4.0-90-generic root=UUID=fb875ad8-746f-48b7-a1c4-c19fc4a7d3ff ro console=ttyS0,115200n8 isolcpu=1-3
[    0.060716] Dentry cache hash table entries: 1048576 (order: 11, 8388608 bytes, linear)
[    0.061674] Inode-cache hash table entries: 524288 (order: 10, 4194304 bytes, linear)
[    0.061838] mem auto-init: stack:off, heap alloc:on, heap free:off
[    0.077318] Calgary: detecting Calgary via BIOS EBDA area
[    0.077321] Calgary: Unable to locate Rio Grande table in EBDA - bailing!
[    0.120897] Memory: 7874788K/8325496K available (14339K kernel code, 2400K rwdata, 5020K rodata, 2736K init, 4964K bss, 450708K reserved, 0K cma-reserved)
[    0.120910] random: get_random_u64 called from kmem_cache_open+0x2d/0x410 with crng_init=0
[    0.121159] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=16, Nodes=1
[    0.121185] ftrace: allocating 44628 entries in 175 pages
[    0.142349] rcu: Hierarchical RCU implementation.
[    0.142354] rcu: 	RCU restricting CPUs from NR_CPUS=8192 to nr_cpu_ids=16.
[    0.142356] 	Tasks RCU enabled.
[    0.142358] rcu: RCU calculated value of scheduler-enlistment delay is 25 jiffies.
[    0.142359] rcu: Adjusting geometry for rcu_fanout_leaf=16, nr_cpu_ids=16
[    0.147073] NR_IRQS: 524544, nr_irqs: 2184, preallocated irqs: 16
[    0.147481] random: crng done (trusting CPU's manufacturer)
[    0.147531] Console: colour dummy device 80x25
[    1.405124] printk: console [ttyS0] enabled
[    1.409463] ACPI: Core revision 20190816
[    1.413680] clocksource: hpet: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 79635855245 ns
[    1.422908] APIC: Switch to symmetric I/O mode setup
[    1.428017] DMAR: Host address width 39
[    1.432000] DMAR: DRHD base: 0x000000fed90000 flags: 0x1
[    1.437465] DMAR: dmar0: reg_base_addr fed90000 ver 1:0 cap d2008c40660462 ecap f050da
[    1.445524] DMAR: RMRR base: 0x0000007eb80000 end: 0x0000007eb9ffff
[    1.451936] DMAR-IR: IOAPIC id 2 under DRHD base  0xfed90000 IOMMU 0
[    1.458431] DMAR-IR: HPET id 0 under DRHD base 0xfed90000
[    1.463974] DMAR-IR: Queued invalidation will be enabled to support x2apic and Intr-remapping.
[    1.473702] DMAR-IR: Enabled IRQ remapping in x2apic mode
[    1.481577] ..TIMER: vector=0x30 apic1=0 pin1=2 apic2=-1 pin2=-1
[    1.506881] clocksource: tsc-early: mask: 0xffffffffffffffff max_cycles: 0x1fb633008a4, max_idle_ns: 440795292230 ns
[    1.517543] Calibrating delay loop (skipped), value calculated using timer frequency.. 4400.00 BogoMIPS (lpj=8800000)
[    1.521541] pid_max: default: 32768 minimum: 301
[    1.535584] LSM: Security Framework initializing
[    1.537566] Yama: becoming mindful.
[    1.541658] AppArmor: AppArmor initialized
[    1.545617] Mount-cache hash table entries: 16384 (order: 5, 131072 bytes, linear)
[    1.549565] Mountpoint-cache hash table entries: 16384 (order: 5, 131072 bytes, linear)
[    1.553568] *** VALIDATE tmpfs ***
[    1.557765] *** VALIDATE proc ***
[    1.561638] *** VALIDATE cgroup1 ***
[    1.565541] *** VALIDATE cgroup2 ***
[    1.569653] mce: CPU0: Thermal monitoring enabled (TM1)
[    1.573627] process: using mwait in idle threads
[    1.577542] Last level iTLB entries: 4KB 48, 2MB 0, 4MB 0
[    1.581539] Last level dTLB entries: 4KB 0, 2MB 0, 4MB 0, 1GB 0
[    1.585544] Spectre V1 : Mitigation: usercopy/swapgs barriers and __user pointer sanitization
[    1.589541] Spectre V2 : Mitigation: Full generic retpoline
[    1.593539] Spectre V2 : Spectre v2 / SpectreRSB mitigation: Filling RSB on context switch
[    1.597539] Spectre V2 : Enabling Restricted Speculation for firmware calls
[    1.601541] Spectre V2 : mitigation: Enabling conditional Indirect Branch Prediction Barrier
[    1.605541] Speculative Store Bypass: Mitigation: Speculative Store Bypass disabled via prctl and seccomp
[    1.609811] Freeing SMP alternatives memory: 40K
[    1.615880] smpboot: CPU0: Intel(R) Atom(TM) CPU C3558 @ 2.20GHz (family: 0x6, model: 0x5f, stepping: 0x1)
[    1.617809] Performance Events: PEBS fmt3+, Goldmont events, 32-deep LBR, full-width counters, Intel PMU driver.
[    1.621542] ... version:                4
[    1.625540] ... bit width:              48
[    1.629540] ... generic registers:      4
[    1.633540] ... value mask:             0000ffffffffffff
[    1.637540] ... max period:             00007fffffffffff
[    1.641539] ... fixed-purpose events:   3
[    1.645540] ... event mask:             000000070000000f
[    1.649614] rcu: Hierarchical SRCU implementation.
[    1.655485] NMI watchdog: Enabled. Permanently consumes one hw-PMU counter.
[    1.657990] smp: Bringing up secondary CPUs ...
[    1.661792] x86: Booting SMP configuration:
[    1.665545] .... node  #0, CPUs:        #1  #2  #3
[    1.677713] smp: Brought up 1 node, 4 CPUs
[    1.685540] smpboot: Max logical packages: 4
[    1.689540] smpboot: Total of 4 processors activated (17600.00 BogoMIPS)
[    1.694664] devtmpfs: initialized
[    1.697609] x86/mm: Memory block size: 128MB
[    1.702854] PM: Registering ACPI NVS region [mem 0x7ebbf000-0x7efbefff] (4194304 bytes)
[    1.705721] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    1.709605] futex hash table entries: 4096 (order: 6, 262144 bytes, linear)
[    1.713652] pinctrl core: initialized pinctrl subsystem
[    1.717702] PM: RTC time: 16:03:07, date: 2021-11-28
[    1.721753] NET: Registered protocol family 16
[    1.725697] audit: initializing netlink subsys (disabled)
[    1.729585] audit: type=2000 audit(1638115385.276:1): state=initialized audit_enabled=0 res=1
[    1.729720] EISA bus registered
[    1.736826] cpuidle: using governor ladder
[    1.737546] cpuidle: using governor menu
[    1.741589] Simple Boot Flag at 0x44 set to 0x1
[    1.745565] ACPI FADT declares the system doesn't support PCIe ASPM, so disable it
[    1.749540] ACPI: bus type PCI registered
[    1.753540] acpiphp: ACPI Hot Plug PCI Controller Driver version: 0.5
[    1.757653] PCI: MMCONFIG for domain 0000 [bus 00-ff] at [mem 0xe0000000-0xefffffff] (base 0xe0000000)
[    1.761559] PCI: MMCONFIG at [mem 0xe0000000-0xefffffff] reserved in E820
[    1.765562] PCI: Using configuration type 1 for base access
[    1.771773] HugeTLB registered 1.00 GiB page size, pre-allocated 0 pages
[    1.773548] HugeTLB registered 2.00 MiB page size, pre-allocated 0 pages
[    1.777680] ACPI: Added _OSI(Module Device)
[    1.781546] ACPI: Added _OSI(Processor Device)
[    1.785543] ACPI: Added _OSI(3.0 _SCP Extensions)
[    1.789549] ACPI: Added _OSI(Processor Aggregator Device)
[    1.793565] ACPI: Added _OSI(Linux-Dell-Video)
[    1.797542] ACPI: Added _OSI(Linux-Lenovo-NV-HDMI-Audio)
[    1.801541] ACPI: Added _OSI(Linux-HPI-Hybrid-Graphics)
[    1.812875] ACPI: 2 ACPI AML tables successfully acquired and loaded
[    1.815114] ACPI: [Firmware Bug]: BIOS _OSI(Linux) query ignored
[    1.818498] ACPI: Dynamic OEM Table Load:
[    1.821554] ACPI: SSDT 0xFFFF914E75ECC300 0000B3 (v02 PmRef  Cpu0Cst  00003001 INTL 20130117)
[    1.826492] ACPI: Dynamic OEM Table Load:
[    1.829546] ACPI: SSDT 0xFFFF914E75F13800 0004B3 (v02 PmRef  Cpu0Ist  00003000 INTL 20130117)
[    1.835215] ACPI: Dynamic OEM Table Load:
[    1.837549] ACPI: SSDT 0xFFFF914E75F16000 00063B (v02 PmRef  ApIst    00003000 INTL 20130117)
[    1.842938] ACPI: Dynamic OEM Table Load:
[    1.845546] ACPI: SSDT 0xFFFF914E75D23400 000231 (v02 PmRef  ApCst    00003000 INTL 20130117)
[    1.851981] ACPI: Interpreter enabled
[    1.853575] ACPI: (supports S0 S4 S5)
[    1.857369] ACPI: Using IOAPIC for interrupt routing
[    1.857595] PCI: Using host bridge windows from ACPI; if necessary, use "pci=nocrs" and report a bug
[    1.861871] ACPI: Enabled 4 GPEs in block 00 to 7F
[    1.876097] ACPI: Power Resource [FN00] (off)
[    1.879009] ACPI: PCI Root Bridge [PCI0] (domain 0000 [bus 00-ff])
[    1.881551] acpi PNP0A08:00: _OSC: OS supports [ExtendedConfig ASPM ClockPM Segments MSI HPX-Type3]
[    1.886103] acpi PNP0A08:00: _OSC: platform does not support [SHPCHotplug LTR]
[    1.890176] acpi PNP0A08:00: _OSC: OS now controls [PCIeHotplug PME AER PCIeCapability]
[    1.893542] acpi PNP0A08:00: FADT indicates ASPM is unsupported, using BIOS configuration
[    1.898293] PCI host bridge to bus 0000:00
[    1.901544] pci_bus 0000:00: root bus resource [io  0x0000-0x0cf7 window]
[    1.905542] pci_bus 0000:00: root bus resource [io  0x0d00-0xffff window]
[    1.909542] pci_bus 0000:00: root bus resource [mem 0x000a0000-0x000bffff window]
[    1.913541] pci_bus 0000:00: root bus resource [mem 0x80000000-0xdfffffff window]
[    1.917542] pci_bus 0000:00: root bus resource [mem 0x280000000-0x7fffffffff window]
[    1.921542] pci_bus 0000:00: root bus resource [bus 00-ff]
[    1.925555] pci 0000:00:00.0: [8086:1980] type 00 class 0x060000
[    1.929757] pci 0000:00:04.0: [8086:19a1] type 00 class 0x060000
[    1.933806] pci 0000:00:05.0: [8086:19a2] type 00 class 0x080700
[    1.937649] pci 0000:00:05.0: PME# supported from D0 D3hot D3cold
[    1.941739] pci 0000:00:06.0: [8086:19a3] type 01 class 0x060400
[    1.945607] pci 0000:00:06.0: PME# supported from D0 D3hot D3cold
[    1.949737] pci 0000:00:0a.0: [8086:19a5] type 01 class 0x060400
[    1.953561] pci 0000:00:0a.0: reg 0x10: [mem 0x81500000-0x8151ffff 64bit]
[    1.957600] pci 0000:00:0a.0: PME# supported from D0 D3hot D3cold
[    1.961736] pci 0000:00:0b.0: [8086:19a6] type 01 class 0x060400
[    1.965560] pci 0000:00:0b.0: reg 0x10: [mem 0x81520000-0x8153ffff 64bit]
[    1.969600] pci 0000:00:0b.0: PME# supported from D0 D3hot D3cold
[    1.973738] pci 0000:00:0c.0: [8086:19a7] type 01 class 0x060400
[    1.977560] pci 0000:00:0c.0: reg 0x10: [mem 0x81540000-0x8155ffff 64bit]
[    1.981600] pci 0000:00:0c.0: PME# supported from D0 D3hot D3cold
[    1.985737] pci 0000:00:0e.0: [8086:19a8] type 01 class 0x060400
[    1.989560] pci 0000:00:0e.0: reg 0x10: [mem 0x81560000-0x8157ffff 64bit]
[    1.993600] pci 0000:00:0e.0: PME# supported from D0 D3hot D3cold
[    1.997762] pci 0000:00:0f.0: [8086:19a9] type 01 class 0x060400
[    2.001560] pci 0000:00:0f.0: reg 0x10: [mem 0x81580000-0x8159ffff 64bit]
[    2.005600] pci 0000:00:0f.0: PME# supported from D0 D3hot D3cold
[    2.009736] pci 0000:00:10.0: [8086:19aa] type 01 class 0x060400
[    2.013561] pci 0000:00:10.0: reg 0x10: [mem 0x815a0000-0x815bffff 64bit]
[    2.017600] pci 0000:00:10.0: PME# supported from D0 D3hot D3cold
[    2.021735] pci 0000:00:11.0: [8086:19ab] type 01 class 0x060400
[    2.025560] pci 0000:00:11.0: reg 0x10: [mem 0x815c0000-0x815dffff 64bit]
[    2.029607] pci 0000:00:11.0: PME# supported from D0 D3hot D3cold
[    2.033743] pci 0000:00:12.0: [8086:19ac] type 00 class 0x088000
[    2.037564] pci 0000:00:12.0: reg 0x10: [mem 0x815f4000-0x815f43ff 64bit]
[    2.041804] pci 0000:00:15.0: [8086:19d0] type 00 class 0x0c0330
[    2.045560] pci 0000:00:15.0: reg 0x10: [mem 0x815e0000-0x815effff 64bit]
[    2.049598] pci 0000:00:15.0: PME# supported from D3hot D3cold
[    2.053733] pci 0000:00:16.0: [8086:19d1] type 01 class 0x060400
[    2.057601] pci 0000:00:16.0: PME# supported from D0 D3hot D3cold
[    2.061728] pci 0000:00:17.0: [8086:19d2] type 01 class 0x060400
[    2.065601] pci 0000:00:17.0: PME# supported from D0 D3hot D3cold
[    2.069732] pci 0000:00:18.0: [8086:19d3] type 00 class 0x078000
[    2.073570] pci 0000:00:18.0: reg 0x10: [mem 0x815f5000-0x815f5fff 64bit]
[    2.077631] pci 0000:00:18.0: PME# supported from D3hot
[    2.081742] pci 0000:00:1c.0: [8086:19db] type 00 class 0x080501
[    2.085564] pci 0000:00:1c.0: reg 0x10: [mem 0x815f6000-0x815f6fff 64bit]
[    2.089552] pci 0000:00:1c.0: reg 0x18: [mem 0x815f7000-0x815f7fff 64bit]
[    2.093767] pci 0000:00:1f.0: [8086:19dc] type 00 class 0x060100
[    2.097789] pci 0000:00:1f.2: [8086:19de] type 00 class 0x058000
[    2.101555] pci 0000:00:1f.2: reg 0x10: [mem 0x815f0000-0x815f3fff]
[    2.105751] pci 0000:00:1f.4: [8086:19df] type 00 class 0x0c0500
[    2.109559] pci 0000:00:1f.4: reg 0x10: [mem 0x815f8000-0x815f80ff 64bit]
[    2.113559] pci 0000:00:1f.4: reg 0x20: [io  0x2000-0x201f]
[    2.117728] pci 0000:00:1f.5: [8086:19e0] type 00 class 0x0c8000
[    2.121556] pci 0000:00:1f.5: reg 0x10: [mem 0xfe010000-0xfe010fff]
[    2.125756] pci 0000:00:1f.7: [8086:19e1] type 00 class 0x130000
[    2.129555] pci 0000:00:1f.7: reg 0x10: [mem 0x00000000-0x000fffff 64bit]
[    2.133547] pci 0000:00:1f.7: reg 0x18: [mem 0xfb000000-0xfb7fffff 64bit]
[    2.137547] pci 0000:00:1f.7: reg 0x20: [mem 0x00000000-0x000007ff 64bit]
[    2.141790] pci 0000:01:00.0: [8086:19e2] type 00 class 0x0b4000
[    2.145574] pci 0000:01:00.0: reg 0x18: [mem 0x80700000-0x8073ffff 64bit]
[    2.149551] pci 0000:01:00.0: reg 0x20: [mem 0x80740000-0x8077ffff 64bit]
[    2.153552] pci 0000:01:00.0: Max Payload Size set to 128 (was 256, max 16384)
[    2.157616] pci 0000:01:00.0: reg 0x164: [mem 0x00000000-0x00000fff 64bit]
[    2.161542] pci 0000:01:00.0: VF(n) BAR0 space: [mem 0x00000000-0x0000ffff 64bit] (contains BAR0 for 16 VFs)
[    2.165549] pci 0000:01:00.0: reg 0x16c: [mem 0x00000000-0x00000fff 64bit]
[    2.169541] pci 0000:01:00.0: VF(n) BAR2 space: [mem 0x00000000-0x0000ffff 64bit] (contains BAR2 for 16 VFs)
[    2.173596] pci 0000:01:00.0: 2.000 Gb/s available PCIe bandwidth, limited by 2.5 GT/s x1 link at 0000:00:06.0 (capable of 64.000 Gb/s with 5 GT/s x16 link)
[    2.177644] pci 0000:00:06.0: PCI bridge to [bus 01]
[    2.181545] pci 0000:00:06.0:   bridge window [mem 0x80700000-0x807fffff]
[    2.185604] pci 0000:00:0a.0: PCI bridge to [bus 11]
[    2.189612] pci 0000:00:0b.0: PCI bridge to [bus 08]
[    2.193623] pci 0000:04:00.0: [8086:15f3] type 00 class 0x020000
[    2.197570] pci 0000:04:00.0: reg 0x10: [mem 0x81300000-0x813fffff]
[    2.201568] pci 0000:04:00.0: reg 0x1c: [mem 0x81400000-0x81403fff]
[    2.205569] pci 0000:04:00.0: reg 0x30: [mem 0xfff00000-0xffffffff pref]
[    2.209622] pci 0000:04:00.0: PME# supported from D0 D3hot D3cold
[    2.213703] pci 0000:00:0c.0: PCI bridge to [bus 04]
[    2.217545] pci 0000:00:0c.0:   bridge window [mem 0x81300000-0x814fffff]
[    2.221621] pci 0000:05:00.0: [8086:15f3] type 00 class 0x020000
[    2.225570] pci 0000:05:00.0: reg 0x10: [mem 0x81100000-0x811fffff]
[    2.229568] pci 0000:05:00.0: reg 0x1c: [mem 0x81200000-0x81203fff]
[    2.233568] pci 0000:05:00.0: reg 0x30: [mem 0xfff00000-0xffffffff pref]
[    2.237622] pci 0000:05:00.0: PME# supported from D0 D3hot D3cold
[    2.241693] pci 0000:00:0e.0: PCI bridge to [bus 05]
[    2.245545] pci 0000:00:0e.0:   bridge window [mem 0x81100000-0x812fffff]
[    2.249623] pci 0000:06:00.0: [8086:15f3] type 00 class 0x020000
[    2.253570] pci 0000:06:00.0: reg 0x10: [mem 0x80f00000-0x80ffffff]
[    2.257568] pci 0000:06:00.0: reg 0x1c: [mem 0x81000000-0x81003fff]
[    2.261569] pci 0000:06:00.0: reg 0x30: [mem 0xfff00000-0xffffffff pref]
[    2.265622] pci 0000:06:00.0: PME# supported from D0 D3hot D3cold
[    2.269698] pci 0000:00:0f.0: PCI bridge to [bus 06]
[    2.273545] pci 0000:00:0f.0:   bridge window [mem 0x80f00000-0x810fffff]
[    2.277621] pci 0000:07:00.0: [8086:15f3] type 00 class 0x020000
[    2.281570] pci 0000:07:00.0: reg 0x10: [mem 0x80d00000-0x80dfffff]
[    2.285569] pci 0000:07:00.0: reg 0x1c: [mem 0x80e00000-0x80e03fff]
[    2.289569] pci 0000:07:00.0: reg 0x30: [mem 0xfff00000-0xffffffff pref]
[    2.293622] pci 0000:07:00.0: PME# supported from D0 D3hot D3cold
[    2.297693] pci 0000:00:10.0: PCI bridge to [bus 07]
[    2.301545] pci 0000:00:10.0:   bridge window [mem 0x80d00000-0x80efffff]
[    2.305607] pci 0000:00:11.0: PCI bridge to [bus 09]
[    2.309626] pci 0000:03:00.0: [8086:15c4] type 00 class 0x020000
[    2.313565] pci 0000:03:00.0: reg 0x10: [mem 0x80400000-0x805fffff 64bit pref]
[    2.317563] pci 0000:03:00.0: reg 0x20: [mem 0x80604000-0x80607fff 64bit pref]
[    2.321548] pci 0000:03:00.0: reg 0x30: [mem 0xfff80000-0xffffffff pref]
[    2.325602] pci 0000:03:00.0: PME# supported from D0 D3hot
[    2.329569] pci 0000:03:00.0: reg 0x184: [mem 0x00000000-0x00003fff 64bit]
[    2.333546] pci 0000:03:00.0: VF(n) BAR0 space: [mem 0x00000000-0x000fffff 64bit] (contains BAR0 for 64 VFs)
[    2.337555] pci 0000:03:00.0: reg 0x190: [mem 0x00000000-0x00003fff 64bit]
[    2.341542] pci 0000:03:00.0: VF(n) BAR3 space: [mem 0x00000000-0x000fffff 64bit] (contains BAR3 for 64 VFs)
[    2.345791] pci 0000:03:00.1: [8086:15c4] type 00 class 0x020000
[    2.349565] pci 0000:03:00.1: reg 0x10: [mem 0x80200000-0x803fffff 64bit pref]
[    2.353563] pci 0000:03:00.1: reg 0x20: [mem 0x80600000-0x80603fff 64bit pref]
[    2.357548] pci 0000:03:00.1: reg 0x30: [mem 0xfff80000-0xffffffff pref]
[    2.361602] pci 0000:03:00.1: PME# supported from D0 D3hot
[    2.365565] pci 0000:03:00.1: reg 0x184: [mem 0x00000000-0x00003fff 64bit]
[    2.369542] pci 0000:03:00.1: VF(n) BAR0 space: [mem 0x00000000-0x000fffff 64bit] (contains BAR0 for 64 VFs)
[    2.373555] pci 0000:03:00.1: reg 0x190: [mem 0x00000000-0x00003fff 64bit]
[    2.377542] pci 0000:03:00.1: VF(n) BAR3 space: [mem 0x00000000-0x000fffff 64bit] (contains BAR3 for 64 VFs)
[    2.381799] pci 0000:00:16.0: PCI bridge to [bus 03]
[    2.385547] pci 0000:00:16.0:   bridge window [mem 0x80200000-0x806fffff 64bit pref]
[    2.389619] pci 0000:02:00.0: [8086:15e5] type 00 class 0x020000
[    2.393564] pci 0000:02:00.0: reg 0x10: [mem 0x80a00000-0x80bfffff 64bit pref]
[    2.397563] pci 0000:02:00.0: reg 0x20: [mem 0x80c04000-0x80c07fff 64bit pref]
[    2.401548] pci 0000:02:00.0: reg 0x30: [mem 0xfff80000-0xffffffff pref]
[    2.405602] pci 0000:02:00.0: PME# supported from D0 D3hot
[    2.409569] pci 0000:02:00.0: reg 0x184: [mem 0x00000000-0x00003fff 64bit]
[    2.413542] pci 0000:02:00.0: VF(n) BAR0 space: [mem 0x00000000-0x000fffff 64bit] (contains BAR0 for 64 VFs)
[    2.417555] pci 0000:02:00.0: reg 0x190: [mem 0x00000000-0x00003fff 64bit]
[    2.421542] pci 0000:02:00.0: VF(n) BAR3 space: [mem 0x00000000-0x000fffff 64bit] (contains BAR3 for 64 VFs)
[    2.425781] pci 0000:02:00.1: [8086:15e5] type 00 class 0x020000
[    2.429565] pci 0000:02:00.1: reg 0x10: [mem 0x80800000-0x809fffff 64bit pref]
[    2.433563] pci 0000:02:00.1: reg 0x20: [mem 0x80c00000-0x80c03fff 64bit pref]
[    2.437548] pci 0000:02:00.1: reg 0x30: [mem 0xfff80000-0xffffffff pref]
[    2.441602] pci 0000:02:00.1: PME# supported from D0 D3hot
[    2.445565] pci 0000:02:00.1: reg 0x184: [mem 0x00000000-0x00003fff 64bit]
[    2.449542] pci 0000:02:00.1: VF(n) BAR0 space: [mem 0x00000000-0x000fffff 64bit] (contains BAR0 for 64 VFs)
[    2.453555] pci 0000:02:00.1: reg 0x190: [mem 0x00000000-0x00003fff 64bit]
[    2.457542] pci 0000:02:00.1: VF(n) BAR3 space: [mem 0x00000000-0x000fffff 64bit] (contains BAR3 for 64 VFs)
[    2.461793] pci 0000:00:17.0: PCI bridge to [bus 02]
[    2.465547] pci 0000:00:17.0:   bridge window [mem 0x80800000-0x80cfffff 64bit pref]
[    2.470292] ACPI: PCI Interrupt Link [LNKA] (IRQs 6 7 10 11 12 14 15) *0, disabled.
[    2.473683] ACPI: PCI Interrupt Link [LNKB] (IRQs 6 7 10 11 12 14 15) *0, disabled.
[    2.477682] ACPI: PCI Interrupt Link [LNKC] (IRQs 6 7 10 11 12 14 15) *0, disabled.
[    2.481681] ACPI: PCI Interrupt Link [LNKD] (IRQs 6 7 10 11 12 14 15) *0, disabled.
[    2.485682] ACPI: PCI Interrupt Link [LNKE] (IRQs 6 7 10 11 12 14 15) *0, disabled.
[    2.489682] ACPI: PCI Interrupt Link [LNKF] (IRQs 6 7 10 11 12 14 15) *0, disabled.
[    2.493682] ACPI: PCI Interrupt Link [LNKG] (IRQs 6 7 10 11 12 14 15) *0, disabled.
[    2.497682] ACPI: PCI Interrupt Link [LNKH] (IRQs 6 7 10 11 12 14 15) *0, disabled.
[    2.502102] iommu: Default domain type: Translated 
[    2.505840] SCSI subsystem initialized
[    2.509579] libata version 3.00 loaded.
[    2.509579] vgaarb: loaded
[    2.512414] ACPI: bus type USB registered
[    2.513567] usbcore: registered new interface driver usbfs
[    2.517551] usbcore: registered new interface driver hub
[    2.521556] usbcore: registered new device driver usb
[    2.525584] pps_core: LinuxPPS API ver. 1 registered
[    2.529541] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    2.533544] PTP clock support registered
[    2.537585] EDAC MC: Ver: 3.0.0
[    2.540971] Registered efivars operations
[    2.541621] PCI: Using ACPI for IRQ routing
[    2.553431] PCI: pci_cache_line_size set to 64 bytes
[    2.553488] pci 0000:00:1f.5: can't claim BAR 0 [mem 0xfe010000-0xfe010fff]: no compatible bridge window
[    2.553585] pci 0000:00:1f.7: can't claim BAR 2 [mem 0xfb000000-0xfb7fffff 64bit]: no compatible bridge window
[    2.557543] e820: reserve RAM buffer [mem 0x0005f000-0x0005ffff]
[    2.557546] e820: reserve RAM buffer [mem 0x71f72018-0x73ffffff]
[    2.557547] e820: reserve RAM buffer [mem 0x71fa4018-0x73ffffff]
[    2.557548] e820: reserve RAM buffer [mem 0x71fd6018-0x73ffffff]
[    2.557549] e820: reserve RAM buffer [mem 0x72008018-0x73ffffff]
[    2.557550] e820: reserve RAM buffer [mem 0x7c2bf000-0x7fffffff]
[    2.557552] e820: reserve RAM buffer [mem 0x7f000000-0x7fffffff]
[    2.557717] NetLabel: Initializing
[    2.561252] NetLabel:  domain hash size = 128
[    2.561541] NetLabel:  protocols = UNLABELED CIPSOv4 CALIPSO
[    2.565559] NetLabel:  unlabeled traffic allowed by default
[    2.571276] hpet0: at MMIO 0xfed00000, IRQs 2, 8, 0, 0, 0, 0, 0, 0
[    2.573552] hpet0: 8 comparators, 64-bit 24.000000 MHz counter
[    2.579608] clocksource: Switched to clocksource tsc-early
[    2.603418] *** VALIDATE bpf ***
[    2.606892] VFS: Disk quotas dquot_6.6.0
[    2.610981] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    2.618035] *** VALIDATE ramfs ***
[    2.621578] *** VALIDATE hugetlbfs ***
[    2.625610] AppArmor: AppArmor Filesystem Enabled
[    2.630494] pnp: PnP ACPI init
[    2.634084] system 00:00: [mem 0xe0000000-0xefffffff] has been reserved
[    2.640838] system 00:00: [mem 0x7f800000-0x7fffffff] has been reserved
[    2.647589] system 00:00: [mem 0xfed60000-0xfed60fff] has been reserved
[    2.654345] system 00:00: Plug and Play ACPI device, IDs PNP0c01 (active)
[    2.654385] pnp 00:01: disabling [mem 0x000c0000-0x000dffff] because it overlaps 0000:00:1f.7 BAR 0 [mem 0x00000000-0x000fffff 64bit]
[    2.666520] pnp 00:01: disabling [mem 0x000e0000-0x000fffff] because it overlaps 0000:00:1f.7 BAR 0 [mem 0x00000000-0x000fffff 64bit]
[    2.678660] pnp 00:01: disabling [mem 0x000c0000-0x000dffff disabled] because it overlaps 0000:03:00.0 BAR 7 [mem 0x00000000-0x000fffff 64bit]
[    2.691575] pnp 00:01: disabling [mem 0x000e0000-0x000fffff disabled] because it overlaps 0000:03:00.0 BAR 7 [mem 0x00000000-0x000fffff 64bit]
[    2.704487] pnp 00:01: disabling [mem 0x000c0000-0x000dffff disabled] because it overlaps 0000:03:00.0 BAR 10 [mem 0x00000000-0x000fffff 64bit]
[    2.717484] pnp 00:01: disabling [mem 0x000e0000-0x000fffff disabled] because it overlaps 0000:03:00.0 BAR 10 [mem 0x00000000-0x000fffff 64bit]
[    2.730486] pnp 00:01: disabling [mem 0x000c0000-0x000dffff disabled] because it overlaps 0000:03:00.1 BAR 7 [mem 0x00000000-0x000fffff 64bit]
[    2.743401] pnp 00:01: disabling [mem 0x000e0000-0x000fffff disabled] because it overlaps 0000:03:00.1 BAR 7 [mem 0x00000000-0x000fffff 64bit]
[    2.756314] pnp 00:01: disabling [mem 0x000c0000-0x000dffff disabled] because it overlaps 0000:03:00.1 BAR 10 [mem 0x00000000-0x000fffff 64bit]
[    2.769312] pnp 00:01: disabling [mem 0x000e0000-0x000fffff disabled] because it overlaps 0000:03:00.1 BAR 10 [mem 0x00000000-0x000fffff 64bit]
[    2.782314] pnp 00:01: disabling [mem 0x000c0000-0x000dffff disabled] because it overlaps 0000:02:00.0 BAR 7 [mem 0x00000000-0x000fffff 64bit]
[    2.795229] pnp 00:01: disabling [mem 0x000e0000-0x000fffff disabled] because it overlaps 0000:02:00.0 BAR 7 [mem 0x00000000-0x000fffff 64bit]
[    2.808140] pnp 00:01: disabling [mem 0x000c0000-0x000dffff disabled] because it overlaps 0000:02:00.0 BAR 10 [mem 0x00000000-0x000fffff 64bit]
[    2.821140] pnp 00:01: disabling [mem 0x000e0000-0x000fffff disabled] because it overlaps 0000:02:00.0 BAR 10 [mem 0x00000000-0x000fffff 64bit]
[    2.834141] pnp 00:01: disabling [mem 0x000c0000-0x000dffff disabled] because it overlaps 0000:02:00.1 BAR 7 [mem 0x00000000-0x000fffff 64bit]
[    2.847063] pnp 00:01: disabling [mem 0x000e0000-0x000fffff disabled] because it overlaps 0000:02:00.1 BAR 7 [mem 0x00000000-0x000fffff 64bit]
[    2.859977] pnp 00:01: disabling [mem 0x000c0000-0x000dffff disabled] because it overlaps 0000:02:00.1 BAR 10 [mem 0x00000000-0x000fffff 64bit]
[    2.872975] pnp 00:01: disabling [mem 0x000e0000-0x000fffff disabled] because it overlaps 0000:02:00.1 BAR 10 [mem 0x00000000-0x000fffff 64bit]
[    2.886014] system 00:01: [io  0x1800-0x187f] has been reserved
[    2.892071] system 00:01: [io  0x0500-0x05fe] has been reserved
[    2.898127] system 00:01: [io  0x0680-0x069f] has been reserved
[    2.904183] system 00:01: [mem 0xfed00000-0xfed003ff] has been reserved
[    2.910931] system 00:01: [mem 0xff800000-0xffffffff] has been reserved
[    2.917685] system 00:01: Plug and Play ACPI device, IDs PNP0c02 (active)
[    2.917726] pnp 00:02: Plug and Play ACPI device, IDs PNP0b00 (active)
[    2.917898] pnp 00:03: Plug and Play ACPI device, IDs PNP0501 (active)
[    2.918071] system 00:04: [io  0x1800-0x18fe] could not be reserved
[    2.924476] system 00:04: [mem 0xfed03000-0xfed03fff] has been reserved
[    2.931232] system 00:04: Plug and Play ACPI device, IDs PNP0c02 (active)
[    2.931577] pnp 00:05: Plug and Play ACPI device, IDs IFX0102 (active)
[    2.931583] pnp: PnP ACPI: found 6 devices
[    2.938601] thermal_sys: Registered thermal governor 'fair_share'
[    2.938602] thermal_sys: Registered thermal governor 'bang_bang'
[    2.944834] thermal_sys: Registered thermal governor 'step_wise'
[    2.950972] thermal_sys: Registered thermal governor 'user_space'
[    2.957115] thermal_sys: Registered thermal governor 'power_allocator'
[    2.967839] clocksource: acpi_pm: mask: 0xffffff max_cycles: 0xffffff, max_idle_ns: 2085701024 ns
[    2.983552] pci 0000:04:00.0: can't claim BAR 6 [mem 0xfff00000-0xffffffff pref]: no compatible bridge window
[    2.993601] pci 0000:05:00.0: can't claim BAR 6 [mem 0xfff00000-0xffffffff pref]: no compatible bridge window
[    3.003649] pci 0000:06:00.0: can't claim BAR 6 [mem 0xfff00000-0xffffffff pref]: no compatible bridge window
[    3.013695] pci 0000:07:00.0: can't claim BAR 6 [mem 0xfff00000-0xffffffff pref]: no compatible bridge window
[    3.023745] pci 0000:03:00.0: can't claim BAR 6 [mem 0xfff80000-0xffffffff pref]: no compatible bridge window
[    3.033790] pci 0000:03:00.1: can't claim BAR 6 [mem 0xfff80000-0xffffffff pref]: no compatible bridge window
[    3.043839] pci 0000:02:00.0: can't claim BAR 6 [mem 0xfff80000-0xffffffff pref]: no compatible bridge window
[    3.053887] pci 0000:02:00.1: can't claim BAR 6 [mem 0xfff80000-0xffffffff pref]: no compatible bridge window
[    3.063938] pci_bus 0000:00: max bus depth: 1 pci_try_num: 2
[    3.069752] pci 0000:00:1f.7: BAR 2: assigned [mem 0x280000000-0x2807fffff 64bit]
[    3.077377] pci 0000:00:16.0: BAR 14: assigned [mem 0x81600000-0x81afffff]
[    3.084388] pci 0000:00:17.0: BAR 14: assigned [mem 0x81b00000-0x81ffffff]
[    3.091402] pci 0000:00:1f.7: BAR 0: assigned [mem 0x280800000-0x2808fffff 64bit]
[    3.099026] pci 0000:00:1f.5: BAR 0: assigned [mem 0x80000000-0x80000fff]
[    3.105958] pci 0000:01:00.0: BAR 7: assigned [mem 0x80780000-0x8078ffff 64bit]
[    3.113405] pci 0000:01:00.0: BAR 9: assigned [mem 0x80790000-0x8079ffff 64bit]
[    3.120852] pci 0000:00:06.0: PCI bridge to [bus 01]
[    3.125956] pci 0000:00:06.0:   bridge window [mem 0x80700000-0x807fffff]
[    3.132884] pci 0000:00:0a.0: PCI bridge to [bus 11]
[    3.137988] pci 0000:00:0b.0: PCI bridge to [bus 08]
[    3.143095] pci 0000:04:00.0: BAR 6: no space for [mem size 0x00100000 pref]
[    3.150281] pci 0000:04:00.0: BAR 6: failed to assign [mem size 0x00100000 pref]
[    3.157810] pci 0000:00:0c.0: PCI bridge to [bus 04]
[    3.162911] pci 0000:00:0c.0:   bridge window [mem 0x81300000-0x814fffff]
[    3.169837] pci 0000:05:00.0: BAR 6: no space for [mem size 0x00100000 pref]
[    3.177020] pci 0000:05:00.0: BAR 6: failed to assign [mem size 0x00100000 pref]
[    3.184550] pci 0000:00:0e.0: PCI bridge to [bus 05]
[    3.189651] pci 0000:00:0e.0:   bridge window [mem 0x81100000-0x812fffff]
[    3.196578] pci 0000:06:00.0: BAR 6: no space for [mem size 0x00100000 pref]
[    3.203760] pci 0000:06:00.0: BAR 6: failed to assign [mem size 0x00100000 pref]
[    3.211290] pci 0000:00:0f.0: PCI bridge to [bus 06]
[    3.216392] pci 0000:00:0f.0:   bridge window [mem 0x80f00000-0x810fffff]
[    3.223318] pci 0000:07:00.0: BAR 6: no space for [mem size 0x00100000 pref]
[    3.230501] pci 0000:07:00.0: BAR 6: failed to assign [mem size 0x00100000 pref]
[    3.238031] pci 0000:00:10.0: PCI bridge to [bus 07]
[    3.243132] pci 0000:00:10.0:   bridge window [mem 0x80d00000-0x80efffff]
[    3.250058] pci 0000:00:11.0: PCI bridge to [bus 09]
[    3.255165] pci 0000:03:00.0: BAR 6: assigned [mem 0x81600000-0x8167ffff pref]
[    3.262524] pci 0000:03:00.1: BAR 6: assigned [mem 0x81680000-0x816fffff pref]
[    3.269881] pci 0000:03:00.0: BAR 7: assigned [mem 0x81700000-0x817fffff 64bit]
[    3.277332] pci 0000:03:00.0: BAR 10: assigned [mem 0x81800000-0x818fffff 64bit]
[    3.284867] pci 0000:03:00.1: BAR 7: assigned [mem 0x81900000-0x819fffff 64bit]
[    3.292317] pci 0000:03:00.1: BAR 10: assigned [mem 0x81a00000-0x81afffff 64bit]
[    3.299849] pci 0000:00:16.0: PCI bridge to [bus 03]
[    3.304954] pci 0000:00:16.0:   bridge window [mem 0x81600000-0x81afffff]
[    3.311884] pci 0000:00:16.0:   bridge window [mem 0x80200000-0x806fffff 64bit pref]
[    3.319793] pci 0000:02:00.0: BAR 6: assigned [mem 0x81b00000-0x81b7ffff pref]
[    3.327161] pci 0000:02:00.1: BAR 6: assigned [mem 0x81b80000-0x81bfffff pref]
[    3.334519] pci 0000:02:00.0: BAR 7: assigned [mem 0x81c00000-0x81cfffff 64bit]
[    3.341971] pci 0000:02:00.0: BAR 10: assigned [mem 0x81d00000-0x81dfffff 64bit]
[    3.349507] pci 0000:02:00.1: BAR 7: assigned [mem 0x81e00000-0x81efffff 64bit]
[    3.356955] pci 0000:02:00.1: BAR 10: assigned [mem 0x81f00000-0x81ffffff 64bit]
[    3.364489] pci 0000:00:17.0: PCI bridge to [bus 02]
[    3.369594] pci 0000:00:17.0:   bridge window [mem 0x81b00000-0x81ffffff]
[    3.376518] pci 0000:00:17.0:   bridge window [mem 0x80800000-0x80cfffff 64bit pref]
[    3.384402] pci_bus 0000:00: resource 4 [io  0x0000-0x0cf7 window]
[    3.390719] pci_bus 0000:00: resource 5 [io  0x0d00-0xffff window]
[    3.397033] pci_bus 0000:00: resource 6 [mem 0x000a0000-0x000bffff window]
[    3.404043] pci_bus 0000:00: resource 7 [mem 0x80000000-0xdfffffff window]
[    3.411053] pci_bus 0000:00: resource 8 [mem 0x280000000-0x7fffffffff window]
[    3.418324] pci_bus 0000:01: resource 1 [mem 0x80700000-0x807fffff]
[    3.424726] pci_bus 0000:04: resource 1 [mem 0x81300000-0x814fffff]
[    3.431127] pci_bus 0000:05: resource 1 [mem 0x81100000-0x812fffff]
[    3.437530] pci_bus 0000:06: resource 1 [mem 0x80f00000-0x810fffff]
[    3.443931] pci_bus 0000:07: resource 1 [mem 0x80d00000-0x80efffff]
[    3.450336] pci_bus 0000:03: resource 1 [mem 0x81600000-0x81afffff]
[    3.456738] pci_bus 0000:03: resource 2 [mem 0x80200000-0x806fffff 64bit pref]
[    3.464097] pci_bus 0000:02: resource 1 [mem 0x81b00000-0x81ffffff]
[    3.470497] pci_bus 0000:02: resource 2 [mem 0x80800000-0x80cfffff 64bit pref]
[    3.478055] NET: Registered protocol family 2
[    3.482780] IP idents hash table entries: 131072 (order: 8, 1048576 bytes, linear)
[    3.492200] tcp_listen_portaddr_hash hash table entries: 4096 (order: 4, 65536 bytes, linear)
[    3.500998] TCP established hash table entries: 65536 (order: 7, 524288 bytes, linear)
[    3.509404] TCP bind hash table entries: 65536 (order: 8, 1048576 bytes, linear)
[    3.517081] TCP: Hash tables configured (established 65536 bind 65536)
[    3.523867] UDP hash table entries: 4096 (order: 5, 131072 bytes, linear)
[    3.530850] UDP-Lite hash table entries: 4096 (order: 5, 131072 bytes, linear)
[    3.538322] NET: Registered protocol family 1
[    3.542824] NET: Registered protocol family 44
[    3.547888] PCI: CLS 64 bytes, default 64
[    3.552131] Trying to unpack rootfs image as initramfs...
[    3.796807] Freeing initrd memory: 50960K
[    3.817567] PCI-DMA: Using software bounce buffering for IO (SWIOTLB)
[    3.824145] software IO TLB: mapped [mem 0x6c7e5000-0x707e5000] (64MB)
[    3.830871] clocksource: tsc: mask: 0xffffffffffffffff max_cycles: 0x1fb633008a4, max_idle_ns: 440795292230 ns
[    3.841026] clocksource: Switched to clocksource tsc
[    3.846252] check: Scanning for low memory corruption every 60 seconds
[    3.853619] Initialise system trusted keyrings
[    3.858219] Key type blacklist registered
[    3.862403] workingset: timestamp_bits=36 max_order=21 bucket_order=0
[    3.870943] zbud: loaded
[    3.874139] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    3.880361] fuse: init (API version 7.31)
[    3.884535] *** VALIDATE fuse ***
[    3.887990] *** VALIDATE fuse ***
[    3.891600] Platform Keyring initialized
[    3.899471] Key type asymmetric registered
[    3.903706] Asymmetric key parser 'x509' registered
[    3.908731] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 244)
[    3.916319] io scheduler mq-deadline registered
[    3.921520] pcieport 0000:00:06.0: PME: Signaling with IRQ 121
[    3.927577] pcieport 0000:00:06.0: AER: enabled with IRQ 121
[    3.933620] pcieport 0000:00:0a.0: PME: Signaling with IRQ 122
[    3.939662] pcieport 0000:00:0a.0: AER: enabled with IRQ 122
[    3.945528] pcieport 0000:00:0a.0: DPC: error containment capabilities: Int Msg #0, RPExt+ PoisonedTLP+ SwTrigger+ RP PIO Log 4, DL_ActiveErr+
[    3.958695] pcieport 0000:00:0b.0: PME: Signaling with IRQ 123
[    3.964736] pcieport 0000:00:0b.0: AER: enabled with IRQ 123
[    3.970600] pcieport 0000:00:0b.0: DPC: error containment capabilities: Int Msg #0, RPExt+ PoisonedTLP+ SwTrigger+ RP PIO Log 4, DL_ActiveErr+
[    3.983773] pcieport 0000:00:0c.0: PME: Signaling with IRQ 124
[    3.989814] pcieport 0000:00:0c.0: AER: enabled with IRQ 124
[    3.995677] pcieport 0000:00:0c.0: DPC: error containment capabilities: Int Msg #0, RPExt+ PoisonedTLP+ SwTrigger+ RP PIO Log 4, DL_ActiveErr+
[    4.008852] pcieport 0000:00:0e.0: PME: Signaling with IRQ 125
[    4.014894] pcieport 0000:00:0e.0: AER: enabled with IRQ 125
[    4.020754] pcieport 0000:00:0e.0: DPC: error containment capabilities: Int Msg #0, RPExt+ PoisonedTLP+ SwTrigger+ RP PIO Log 4, DL_ActiveErr+
[    4.033938] pcieport 0000:00:0f.0: PME: Signaling with IRQ 126
[    4.039985] pcieport 0000:00:0f.0: AER: enabled with IRQ 126
[    4.045867] pcieport 0000:00:0f.0: DPC: error containment capabilities: Int Msg #0, RPExt+ PoisonedTLP+ SwTrigger+ RP PIO Log 4, DL_ActiveErr+
[    4.059057] pcieport 0000:00:10.0: PME: Signaling with IRQ 127
[    4.065100] pcieport 0000:00:10.0: AER: enabled with IRQ 127
[    4.070963] pcieport 0000:00:10.0: DPC: error containment capabilities: Int Msg #0, RPExt+ PoisonedTLP+ SwTrigger+ RP PIO Log 4, DL_ActiveErr+
[    4.084136] pcieport 0000:00:11.0: PME: Signaling with IRQ 128
[    4.090177] pcieport 0000:00:11.0: AER: enabled with IRQ 128
[    4.096038] pcieport 0000:00:11.0: DPC: error containment capabilities: Int Msg #0, RPExt+ PoisonedTLP+ SwTrigger+ RP PIO Log 4, DL_ActiveErr+
[    4.109203] pcieport 0000:00:16.0: PME: Signaling with IRQ 129
[    4.115251] pcieport 0000:00:16.0: AER: enabled with IRQ 129
[    4.121269] pcieport 0000:00:17.0: PME: Signaling with IRQ 130
[    4.127311] pcieport 0000:00:17.0: AER: enabled with IRQ 130
[    4.133169] shpchp: Standard Hot Plug PCI Controller Driver version: 0.4
[    4.140096] intel_idle: MWAIT substates: 0x2020
[    4.140098] intel_idle: v0.4.1 model 0x5F
[    4.140367] intel_idle: lapic_timer_reliable_states 0xffffffff
[    4.140517] input: Power Button as /devices/LNXSYSTM:00/LNXSYBUS:00/PNP0C0C:00/input/input0
[    4.149039] ACPI: Power Button [PWRB]
[    4.152884] input: Power Button as /devices/LNXSYSTM:00/LNXPWRBN:00/input/input1
[    4.160468] ACPI: Power Button [PWRF]
[    4.165649] thermal LNXTHERM:00: registered as thermal_zone0
[    4.171448] ACPI: Thermal Zone [TZ01] (27 C)
[    4.176059] Serial: 8250/16550 driver, 32 ports, IRQ sharing enabled
[    4.202810] 00:03: ttyS0 at I/O 0x3f8 (irq = 16, base_baud = 115200) is a 16550A
[    4.212928] Linux agpgart interface v0.103
[    4.219699] tpm_tis 00:05: 2.0 TPM (device-id 0x1B, rev-id 22)
[    4.227867] tpm tpm0: A TPM error (256) occurred attempting the self test
[    4.234798] tpm tpm0: starting up the TPM manually
[    4.953613] loop: module loaded
[    4.957296] libphy: Fixed MDIO Bus: probed
[    4.961534] tun: Universal TUN/TAP device driver, 1.6
[    4.966837] PPP generic driver version 2.4.2
[    4.971460] VFIO - User Level meta-driver version: 0.3
[    4.976918] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver
[    4.983588] ehci-pci: EHCI PCI platform driver
[    4.988187] ehci-platform: EHCI generic platform driver
[    4.993556] ohci_hcd: USB 1.1 'Open' Host Controller (OHCI) Driver
[    4.999872] ohci-pci: OHCI PCI platform driver
[    5.004462] ohci-platform: OHCI generic platform driver
[    5.009829] uhci_hcd: USB Universal Host Controller Interface driver
[    5.016599] xhci_hcd 0000:00:15.0: xHCI Host Controller
[    5.021967] xhci_hcd 0000:00:15.0: new USB bus registered, assigned bus number 1
[    5.030571] xhci_hcd 0000:00:15.0: hcc params 0x200077c1 hci version 0x100 quirks 0x0000000001109810
[    5.039871] xhci_hcd 0000:00:15.0: cache line size of 64 is not supported
[    5.047041] xhci_hcd 0000:00:15.0: xHCI Host Controller
[    5.052404] xhci_hcd 0000:00:15.0: new USB bus registered, assigned bus number 2
[    5.059938] xhci_hcd 0000:00:15.0: Host supports USB 3.0 SuperSpeed
[    5.066392] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 5.04
[    5.074796] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    5.082153] usb usb1: Product: xHCI Host Controller
[    5.087166] usb usb1: Manufacturer: Linux 5.4.0-90-generic xhci-hcd
[    5.093567] usb usb1: SerialNumber: 0000:00:15.0
[    5.098540] hub 1-0:1.0: USB hub found
[    5.102445] hub 1-0:1.0: 4 ports detected
[    5.107569] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 5.04
[    5.115973] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    5.123329] usb usb2: Product: xHCI Host Controller
[    5.128343] usb usb2: Manufacturer: Linux 5.4.0-90-generic xhci-hcd
[    5.134746] usb usb2: SerialNumber: 0000:00:15.0
[    5.139650] hub 2-0:1.0: USB hub found
[    5.143547] hub 2-0:1.0: 4 ports detected
[    5.148689] i8042: PNP: No PS/2 controller found.
[    5.153670] mousedev: PS/2 mouse device common for all mice
[    5.159618] rtc_cmos 00:02: RTC can wake from S4
[    5.164710] rtc_cmos 00:02: registered as rtc0
[    5.169313] rtc_cmos 00:02: alarms up to one month, 242 bytes nvram, hpet irqs
[    5.176684] i2c /dev entries driver
[    5.180372] device-mapper: uevent: version 1.0.3
[    5.185239] device-mapper: ioctl: 4.41.0-ioctl (2019-09-16) initialised: dm-devel@redhat.com
[    5.193839] platform eisa.0: Probing EISA bus 0
[    5.198504] platform eisa.0: EISA: Cannot allocate resource for mainboard
[    5.205425] platform eisa.0: Cannot allocate resource for EISA slot 1
[    5.212007] platform eisa.0: Cannot allocate resource for EISA slot 2
[    5.218581] platform eisa.0: Cannot allocate resource for EISA slot 3
[    5.225157] platform eisa.0: Cannot allocate resource for EISA slot 4
[    5.231732] platform eisa.0: Cannot allocate resource for EISA slot 5
[    5.238308] platform eisa.0: Cannot allocate resource for EISA slot 6
[    5.244884] platform eisa.0: Cannot allocate resource for EISA slot 7
[    5.251459] platform eisa.0: Cannot allocate resource for EISA slot 8
[    5.258035] platform eisa.0: EISA: Detected 0 cards
[    5.263048] intel_pstate: CPU model not supported
[    5.268028] ledtrig-cpu: registered to indicate activity on CPUs
[    5.274175] EFI Variables Facility v0.08 2004-May-17
[    5.372046] drop_monitor: Initializing network drop monitor service
[    5.378704] NET: Registered protocol family 10
[    5.391874] Segment Routing with IPv6
[    5.395701] NET: Registered protocol family 17
[    5.400356] Key type dns_resolver registered
[    5.405418] RAS: Correctable Errors collector initialized.
[    5.411112] microcode: sig=0x506f1, pf=0x1, revision=0x34
[    5.416663] usb 2-2: new SuperSpeed Gen 1 USB device number 2 using xhci_hcd
[    5.421783] microcode: Microcode Update Driver: v2.2.
[    5.424054] *** VALIDATE rdt ***
[    5.432624] resctrl: L2 allocation detected
[    5.436944] IPI shorthand broadcast: enabled
[    5.441360] sched_clock: Marking stable (4135131832, 1306215697)->(6150381162, -709033633)
[    5.449967] registered taskstats version 1
[    5.454220] Loading compiled-in X.509 certificates
[    5.454575] usb 2-2: New USB device found, idVendor=0781, idProduct=5583, bcdDevice= 1.00
[    5.467468] usb 2-2: New USB device strings: Mfr=1, Product=2, SerialNumber=3
[    5.474741] usb 2-2: Product: Ultra Fit
[    5.478711] usb 2-2: Manufacturer: SanDisk
[    5.482942] usb 2-2: SerialNumber: 0101be85b067ca0d703486a24a44646525df8e76c47edeadf7b9c53e084d130ff85a00000000000000000000c0e69e70000319008355810797264240
[    5.498346] Loaded X.509 cert 'Build time autogenerated kernel key: 85cd93e325e502cfcb4258a2209a1e273ffd77af'
[    5.509570] Loaded X.509 cert 'Canonical Ltd. Live Patch Signing: 14df34d1a87cf37625abec039ef2bf521249b969'
[    5.520613] Loaded X.509 cert 'Canonical Ltd. Kernel Module Signing: 88f752e560a1e0737e31163a466ad7b70a850c19'
[    5.530798] zswap: loaded using pool lzo/zbud
[    5.535517] Key type ._fscrypt registered
[    5.539668] Key type .fscrypt registered
[    5.552293] Key type big_key registered
[    5.556272] Key type trusted registered
[    5.564271] Key type encrypted registered
[    5.568422] AppArmor: AppArmor sha1 policy hashing enabled
[    5.575535] integrity: Loading X.509 certificate: UEFI:MokListRT
[    5.582377] integrity: Loaded X.509 cert 'Canonical Ltd. Master Certificate Authority: ad91990bc22ab1f517048c23b6655a268e345a63'
[    5.594910] ima: Allocated hash algorithm: sha1
[    5.634717] ima: No architecture policies found
[    5.639398] evm: Initialising EVM extended attributes:
[    5.644670] evm: security.selinux
[    5.648119] evm: security.SMACK64
[    5.651570] evm: security.SMACK64EXEC
[    5.655366] evm: security.SMACK64TRANSMUTE
[    5.659594] evm: security.SMACK64MMAP
[    5.663387] evm: security.apparmor
[    5.666921] evm: security.ima
[    5.670019] evm: security.capability
[    5.673726] evm: HMAC attrs: 0x1
[    5.677726] PM:   Magic number: 13:346:86
[    5.682069] rtc_cmos 00:02: setting system clock to 2021-11-28T16:03:12 UTC (1638115392)
[    5.693475] Freeing unused decrypted memory: 2040K
[    5.699416] Freeing unused kernel image memory: 2736K
[    5.704648] Write protecting the kernel read-only data: 22528k
[    5.711669] Freeing unused kernel image memory: 2008K
[    5.717328] Freeing unused kernel image memory: 1124K
[    5.741240] x86/mm: Checked W+X mappings: passed, no W+X pages found.
[    5.747817] Run /init as init process
[    5.883323] Intel(R) 2.5G Ethernet Linux Driver - version 0.0.1-k
[    5.889573] Copyright(c) 2018 Intel Corporation.
[    5.903398] usb-storage 2-2:1.0: USB Mass Storage device detected
[    5.935053] dca service started, version 1.12.1
[    5.939747] scsi host0: usb-storage 2-2:1.0
[    5.944476] i801_smbus 0000:00:1f.4: SMBus using PCI interrupt
[    5.944514] usbcore: registered new interface driver usb-storage
[    5.957374] sdhci: Secure Digital Host Controller Interface driver
[    5.963706] sdhci: Copyright(c) Pierre Ossman
[    5.972629] ixgbe: Intel(R) 10 Gigabit PCI Express Network Driver - version 5.1.0-k
[    5.980435] ixgbe: Copyright (c) 1999-2016 Intel Corporation.
[    5.986567] sdhci-pci 0000:00:1c.0: SDHCI controller found [8086:19db] (rev 11)
[    5.987680] usbcore: registered new interface driver uas
[    5.994575] mmc0: SDHCI controller on PCI [0000:00:1c.0] using ADMA 64-bit
[    6.041061] igc 0000:04:00.0: 4.000 Gb/s available PCIe bandwidth (5 GT/s x1 link)
[    6.048786] igc 0000:04:00.0 eth0: MAC: 90:ec:77:1b:63:55
[    6.128664] mmc0: new HS400 MMC card at address 0001
[    6.137188] mmcblk0: mmc0:0001 TB2916 14.6 GiB 
[    6.142039] mmcblk0boot0: mmc0:0001 TB2916 partition 1 4.00 MiB
[    6.148258] mmcblk0boot1: mmc0:0001 TB2916 partition 2 4.00 MiB
[    6.154445] mmcblk0rpmb: mmc0:0001 TB2916 partition 3 4.00 MiB, chardev (241:0)
[    6.157804] igc 0000:05:00.0: 4.000 Gb/s available PCIe bandwidth (5 GT/s x1 link)
[    6.169613] igc 0000:05:00.0 eth1: MAC: 90:ec:77:1b:63:56
[    6.197134]  mmcblk0: p1 p2
[    6.278959] igc 0000:06:00.0: 4.000 Gb/s available PCIe bandwidth (5 GT/s x1 link)
[    6.286680] igc 0000:06:00.0 eth2: MAC: 90:ec:77:1b:63:57
[    6.393013] igc 0000:07:00.0: 4.000 Gb/s available PCIe bandwidth (5 GT/s x1 link)
[    6.398151] ixgbe 0000:03:00.0: Multiqueue Enabled: Rx Queue count = 4, Tx Queue count = 4 XDP Queue count = 0
[    6.400727] igc 0000:07:00.0 eth3: MAC: 90:ec:77:1b:63:58
[    6.417807] igc 0000:05:00.0 enp5s0: renamed from eth1
[    6.505720] igc 0000:04:00.0 enp4s0: renamed from eth0
[    6.529932] igc 0000:06:00.0 enp6s0: renamed from eth2
[    6.545579] ixgbe 0000:03:00.0: MAC: 6, PHY: 20, SFP+: 5, PBA No: 000500-000
[    6.552767] ixgbe 0000:03:00.0: 90:ec:77:1b:63:53
[    6.598194] igc 0000:07:00.0 enp7s0: renamed from eth3
[    6.689043] ixgbe 0000:03:00.0: Intel(R) 10 Gigabit Network Connection
[    6.695771] libphy: ixgbe-mdio: probed
[    6.954749] scsi 0:0:0:0: Direct-Access     SanDisk  Ultra Fit        1.00 PQ: 0 ANSI: 6
[    6.963630] sd 0:0:0:0: [sda] 240353280 512-byte logical blocks: (123 GB/115 GiB)
[    6.963858] sd 0:0:0:0: Attached scsi generic sg0 type 0
[    6.977377] sd 0:0:0:0: [sda] Write Protect is off
[    6.982310] sd 0:0:0:0: [sda] Mode Sense: 43 00 00 00
[    6.982705] sd 0:0:0:0: [sda] Write cache: disabled, read cache: enabled, doesn't support DPO or FUA
[    7.015084]  sda: sda1 sda2 sda3
                sda2: <bsd: sda5 >
[    7.040355] sd 0:0:0:0: [sda] Attached SCSI removable disk
[    7.109706] ixgbe 0000:03:00.1: Multiqueue Enabled: Rx Queue count = 4, Tx Queue count = 4 XDP Queue count = 0
[    7.245591] ixgbe 0000:03:00.1: MAC: 6, PHY: 20, SFP+: 6, PBA No: 000500-000
[    7.252781] ixgbe 0000:03:00.1: 90:ec:77:1b:63:54
[    7.390593] ixgbe 0000:03:00.1: Intel(R) 10 Gigabit Network Connection
[    7.738313] ixgbe 0000:02:00.0: Multiqueue Enabled: Rx Queue count = 4, Tx Queue count = 4 XDP Queue count = 0
[    7.875646] ixgbe 0000:02:00.0: MAC: 6, PHY: 27, PBA No: 000800-000
[    7.882051] ixgbe 0000:02:00.0: 90:ec:77:1b:63:52
[    7.931041] ixgbe 0000:02:00.0: Intel(R) 10 Gigabit Network Connection
[    8.278280] ixgbe 0000:02:00.1: Multiqueue Enabled: Rx Queue count = 4, Tx Queue count = 4 XDP Queue count = 0
[    8.415646] ixgbe 0000:02:00.1: MAC: 6, PHY: 27, PBA No: 000800-000
[    8.422054] ixgbe 0000:02:00.1: 90:ec:77:1b:63:51
[    8.471042] ixgbe 0000:02:00.1: Intel(R) 10 Gigabit Network Connection
[    8.479255] ixgbe 0000:03:00.0 enp3s0f0: renamed from eth0
[    8.513712] ixgbe 0000:03:00.1 enp3s0f1: renamed from eth1
[    8.533927] ixgbe 0000:02:00.0 enp2s0f0: renamed from eth2
[    8.557745] ixgbe 0000:02:00.1 enp2s0f1: renamed from eth3
[    9.611309] EXT4-fs (mmcblk0p2): mounted filesystem with ordered data mode. Opts: (null)
[    9.835166] systemd[1]: Inserted module 'autofs4'
[   10.013538] systemd[1]: systemd 245.4-4ubuntu3.13 running in system mode. (+PAM +AUDIT +SELINUX +IMA +APPARMOR +SMACK +SYSVINIT +UTMP +LIBCRYPTSETUP +GCRYPT +GNUTLS +ACL +XZ +LZ4 +SECCOMP +BLKID +ELFUTILS +KMOD +IDN2 -IDN +PCRE2 default-hierarchy=hybrid)
[   10.053671] systemd[1]: Detected architecture x86-64.
[   10.133923] systemd[1]: Set hostname to <netgate>.
[   10.387340] systemd[1]: Created slice system-modprobe.slice.
[   10.410015] systemd[1]: Created slice system-serial\x2dgetty.slice.
[   10.433960] systemd[1]: Created slice system-systemd\x2dfsck.slice.
[   10.458064] systemd[1]: Created slice User and Session Slice.
[   10.481706] systemd[1]: Started Forward Password Requests to Wall Directory Watch.
[   10.506029] systemd[1]: Set up automount Arbitrary Executable File Formats File System Automount Point.
[   10.533696] systemd[1]: Reached target User and Group Name Lookups.
[   10.557633] systemd[1]: Reached target Remote File Systems.
[   10.577624] systemd[1]: Reached target Slices.
[   10.597807] systemd[1]: Listening on Syslog Socket.
[   10.617745] systemd[1]: Listening on fsck to fsckd communication Socket.
[   10.641695] systemd[1]: Listening on initctl Compatibility Named Pipe.
[   10.665907] systemd[1]: Listening on Journal Audit Socket.
[   10.685737] systemd[1]: Listening on Journal Socket (/dev/log).
[   10.709773] systemd[1]: Listening on Journal Socket.
[   10.729768] systemd[1]: Listening on udev Control Socket.
[   10.749712] systemd[1]: Listening on udev Kernel Socket.
[   10.771012] systemd[1]: Mounting Huge Pages File System...
[   10.790987] systemd[1]: Mounting POSIX Message Queue File System...
[   10.814884] systemd[1]: Mounting Kernel Debug File System...
[   10.834920] systemd[1]: Mounting Kernel Trace File System...
[   10.855743] systemd[1]: Starting Journal Service...
[   10.875249] systemd[1]: Starting Set the console keyboard layout...
[   10.899107] systemd[1]: Starting Create list of static device nodes for the current kernel...
[   10.928000] systemd[1]: Starting Load Kernel Module drm...
[   10.949633] systemd[1]: Condition check resulted in OpenVSwitch configuration for cleanup being skipped.
[   10.962530] systemd[1]: Condition check resulted in Set Up Additional Binary Formats being skipped.
[   10.971754] systemd[1]: Condition check resulted in File System Check on Root Device being skipped.
[   10.982934] systemd[1]: Starting Load Kernel Modules...
[   11.002978] systemd[1]: Starting Remount Root and Kernel File Systems...
[   11.020283] EXT4-fs (mmcblk0p2): re-mounted. Opts: errors=remount-ro
[   11.028330] systemd[1]: Starting udev Coldplug all Devices...
[   11.050897] systemd[1]: Starting Uncomplicated firewall...
[   11.079771] systemd[1]: Started Journal Service.
[   11.320291] systemd-journald[274]: Received client request to flush runtime journal.
[   11.345670] Adding 684488k swap on /swapfile.  Priority:-2 extents:3 across:700872k SSFS
[   12.128786] intel_th_pci 0000:00:1f.7: enabling device (0000 -> 0002)
[   12.222398] RAPL PMU: API unit is 2^-32 Joules, 2 fixed counters, 655360 ms ovfl timer
[   12.222402] RAPL PMU: hw unit of domain pp0-core 2^-14 Joules
[   12.222403] RAPL PMU: hw unit of domain package 2^-14 Joules
[   12.237418] cryptd: max_cpu_qlen set to 1000
[   12.276796] SSE version of gcm_enc/dec engaged.
[   12.414799] EDAC pnd2: ECC disabled on channel 0
[   12.414801] EDAC pnd2: Failed to register device with error -22.
[   12.458330] EDAC pnd2: ECC disabled on channel 0
[   12.458332] EDAC pnd2: Failed to register device with error -22.
[   12.468652] intel_rapl_common: Found RAPL domain package
[   12.468655] intel_rapl_common: Found RAPL domain core
[   12.504777] pps pps0: new PPS source ptp0
[   12.504835] ixgbe 0000:02:00.1: registered PHC device on enp2s0f1
[   12.514098] EDAC pnd2: ECC disabled on channel 0
[   12.514100] EDAC pnd2: Failed to register device with error -22.
[   12.555917] EDAC pnd2: ECC disabled on channel 0
[   12.555919] EDAC pnd2: Failed to register device with error -22.
[   12.574272] audit: type=1400 audit(1638115399.387:2): apparmor="STATUS" operation="profile_load" profile="unconfined" name="nvidia_modprobe" pid=390 comm="apparmor_parser"
[   12.574278] audit: type=1400 audit(1638115399.387:3): apparmor="STATUS" operation="profile_load" profile="unconfined" name="nvidia_modprobe//kmod" pid=390 comm="apparmor_parser"
[   12.575222] audit: type=1400 audit(1638115399.387:4): apparmor="STATUS" operation="profile_load" profile="unconfined" name="/usr/bin/man" pid=391 comm="apparmor_parser"
[   12.575227] audit: type=1400 audit(1638115399.387:5): apparmor="STATUS" operation="profile_load" profile="unconfined" name="man_filter" pid=391 comm="apparmor_parser"
[   12.575230] audit: type=1400 audit(1638115399.387:6): apparmor="STATUS" operation="profile_load" profile="unconfined" name="man_groff" pid=391 comm="apparmor_parser"
[   12.580389] audit: type=1400 audit(1638115399.391:7): apparmor="STATUS" operation="profile_load" profile="unconfined" name="/usr/sbin/tcpdump" pid=389 comm="apparmor_parser"
[   12.581030] audit: type=1400 audit(1638115399.391:8): apparmor="STATUS" operation="profile_load" profile="unconfined" name="lsb_release" pid=393 comm="apparmor_parser"
[   12.584323] audit: type=1400 audit(1638115399.395:9): apparmor="STATUS" operation="profile_load" profile="unconfined" name="/usr/lib/NetworkManager/nm-dhcp-client.action" pid=388 comm="apparmor_parser"
[   12.584329] audit: type=1400 audit(1638115399.395:10): apparmor="STATUS" operation="profile_load" profile="unconfined" name="/usr/lib/NetworkManager/nm-dhcp-helper" pid=388 comm="apparmor_parser"
[   12.584332] audit: type=1400 audit(1638115399.395:11): apparmor="STATUS" operation="profile_load" profile="unconfined" name="/usr/lib/connman/scripts/dhclient-script" pid=388 comm="apparmor_parser"
[   12.621603] c3xxx 0000:01:00.0: qat_dev0 started 6 acceleration engines
[   12.705744] pps pps1: new PPS source ptp1
[   12.705833] ixgbe 0000:03:00.1: registered PHC device on enp3s0f1
[   12.729225] pps pps2: new PPS source ptp2
[   12.730286] ixgbe 0000:03:00.0: registered PHC device on enp3s0f0
[   12.811570] ixgbe 0000:03:00.1 enp3s0f1: detected SFP+: 6
[   13.449589] ixgbe 0000:03:00.1 enp3s0f1: NIC Link is Up 10 Gbps, Flow Control: RX/TX
[   13.449810] IPv6: ADDRCONF(NETDEV_CHANGE): enp3s0f1: link becomes ready
[   13.463834] ixgbe 0000:02:00.1 enp2s0f1: NIC Link is Up 1 Gbps, Flow Control: RX/TX
[   13.464339] IPv6: ADDRCONF(NETDEV_CHANGE): enp2s0f1: link becomes ready
[   13.565590] ixgbe 0000:03:00.0 enp3s0f0: detected SFP+: 5
[   13.569853] IPMI message handler: version 39.2
[   13.572505] ipmi device interface
[   13.583677] ipmi_si: IPMI System Interface driver
[   13.583792] ipmi_si: Unable to find any System Interface(s)
[   14.136217] fbcon: Taking over console
[   14.213621] ixgbe 0000:03:00.0 enp3s0f0: NIC Link is Up 10 Gbps, Flow Control: RX/TX
[   14.214392] IPv6: ADDRCONF(NETDEV_CHANGE): enp3s0f0: link becomes ready
